A B C D E F G H I K L M O P Q R S T V W X

## A

AccessPassword - Static variable in class com.impinj.octane.WordPointers
  The 2-word access password is stored at this word in reserved memory
add(Object) - Method in class com.impinj.octane.AntennaConfigGroup
add(Object) - Method in class com.impinj.octane.AntennaHubStatusGroup
Add(Object) - Method in class com.impinj.octane.AntennaStatusGroup
add(Object) - Method in class com.impinj.octane.GpiConfigGroup
add(Object) - Method in class com.impinj.octane.GpiStatusGroup
add(Object) - Method in class com.impinj.octane.GpoConfigGroup
add(LLRPMessage) - Method in class com.impinj.octane.ImpinjReader.MessageHandler
addMetric(Integer) - Method in class com.impinj.octane.DiagnosticReport
addOpSequence(TagOpSequence) - Method in class com.impinj.octane.ImpinjReader
  Adds a sequence of tag operations to the reader to perform during inventory
addResult(TagOpResult) - Method in class com.impinj.octane.TagOpReport
addTag(Tag) - Method in class com.impinj.octane.TagReport
AdjustPcBits(short, short) - Static method in class com.impinj.octane.PcBits
  Returns new PC bits, based on the current PC bits and the new EPC length.
All - Static variable in class com.impinj.octane.AntennaIds
  All antennas
AntennaChangeListener - Interface in com.impinj.octane
  Your application can implement this interface to receive antenna change events.
AntennaConfig - Class in com.impinj.octane
  This class hold the antenna configuration information.
AntennaConfig(Number) - Constructor for class com.impinj.octane.AntennaConfig
  Constructor for a new antenna configuration object.
AntennaConfigGroup - Class in com.impinj.octane
  This class hold the collection of antenna configuration.
AntennaEvent - Class in com.impinj.octane
  This class contains the information about a change in antenna state.
AntennaEvent() - Constructor for class com.impinj.octane.AntennaEvent
AntennaEventType - Enum in com.impinj.octane
  The reader uses an internal mechanism to detect whether antennas are connected or disconnected from each antenna port.
AntennaHubStatus - Class in com.impinj.octane
  Speedway Revolution readers can be outfitted with antenna hubs which allows the reader to operate more antenna ports.
AntennaHubStatus() - Constructor for class com.impinj.octane.AntennaHubStatus
AntennaHubStatusGroup - Class in com.impinj.octane
  Contains the collection of antenna Hub status for the antenna hubs connected to the ImpinjReader.
AntennaIds - Class in com.impinj.octane
  Helper class used when identifying that all antennas should be used when configuring a tag operation.
AntennaIds() - Constructor for class com.impinj.octane.AntennaIds
AntennaStatus - Class in com.impinj.octane
  Class containing The status information for an individual antenna port.
AntennaStatus() - Constructor for class com.impinj.octane.AntennaStatus
AntennaStatusGroup - Class in com.impinj.octane
  The collection of antenna statuses for the readers antennas
AntennaUtilities - Class in com.impinj.octane
  Static class that provides utility functions for getting antenna patterns.
applyDefaultSettings() - Method in class com.impinj.octane.ImpinjReader
  Applies the default settings to the reader.
applySettings(SET_READER_CONFIG, ADD_ROSPEC) - Method in class com.impinj.octane.ImpinjReader
  Applies the provided settings to the reader.
applySettings(Settings) - Method in class com.impinj.octane.ImpinjReader
  Applies the provided settings to the reader.
AutoStartConfig - Class in com.impinj.octane
  The ImpinjReader can be configured to start inventory automatically based on several inputs including General purpose input (GPI) and time.
AutoStartConfig() - Constructor for class com.impinj.octane.AutoStartConfig
AutoStartMode - Enum in com.impinj.octane
  The ImpinjReader can be configured to start inventory automatically based on several inputs including General purpose input (GPI) and time.
AutoStopConfig - Class in com.impinj.octane
  The ImpinjReader can be configured to stop inventory automatically based on several inputs including General purpose input (GPI) and time.
AutoStopConfig() - Constructor for class com.impinj.octane.AutoStopConfig
AutoStopMode - Enum in com.impinj.octane
  The ImpinjReader can be configured to stop inventory automatically based on several inputs including General purpose input (GPI) and time.

## B

BackgroundWorker - Class in com.impinj.octane
  An internal class that is currently unused
BackgroundWorker(int) - Constructor for class com.impinj.octane.BackgroundWorker
BitPointers - Class in com.impinj.octane
  These constants point to bit locations in memory for common fields.
BitPointers() - Constructor for class com.impinj.octane.BitPointers
BlockPermalockMask - Class in com.impinj.octane
  Uses to specify which blocks to permalock.
BlockPermalockMask() - Constructor for class com.impinj.octane.BlockPermalockMask
BlockPermalockResult - Enum in com.impinj.octane
  An enumeration to hold the block permalock result.
BufferOverflowEvent - Class in com.impinj.octane
  This event carries information on a buffer overflow event.
BufferOverflowEvent() - Constructor for class com.impinj.octane.BufferOverflowEvent
BufferOverflowListener - Interface in com.impinj.octane
  Your application can implement this interface to receive buffer overflow events.
BufferWarningEvent - Class in com.impinj.octane
  This class holds the buffer warning event information.
BufferWarningEvent() - Constructor for class com.impinj.octane.BufferWarningEvent
BufferWarningListener - Interface in com.impinj.octane
  Your application can implement this interface to receive buffer warnings.
buildAddROSpecMessage(Settings) - Method in class com.impinj.octane.ImpinjReader
  Build up an LTK add ROSpec message.
buildSetReaderConfigMessage(Settings) - Method in class com.impinj.octane.ImpinjReader
  Build up an LTK set reader config message.

## C

close() - Method in class com.impinj.octane.RshellEngine
  Closes an rshell connection to the readers
Close() - Method in interface com.impinj.octane.RShellSocket
Close() - Method in class com.impinj.octane.SshRShellSocket
Close() - Method in class com.impinj.octane.TelnetRShellSocket
com.impinj.octane - package com.impinj.octane
CommunicationsStandardType - Enum in com.impinj.octane
  This enumerations defines the regulatory rules under which this device operates
connect() - Method in class com.impinj.octane.ImpinjReader
  Connect (unsecured) to an Impinj RFID reader using the default LLRP port (5084).
connect(String) - Method in class com.impinj.octane.ImpinjReader
  Connect (unsecured) to an Impinj RFID reader using the default LLRP port (5084).
connect(String, boolean) - Method in class com.impinj.octane.ImpinjReader
  Connect to an Impinj RFID reader using the default LLRP port (5084).
connect(String, int) - Method in class com.impinj.octane.ImpinjReader
  Connect (unsecured) to an Impinj RFID reader.
connect(String, int, boolean) - Method in class com.impinj.octane.ImpinjReader
  Connect to an Impinj RFID reader.
Connect() - Method in interface com.impinj.octane.RShellSocket
Connect() - Method in class com.impinj.octane.SshRShellSocket
Connect() - Method in class com.impinj.octane.TelnetRShellSocket
ConnectAsyncResult - Enum in com.impinj.octane
  Enumeration used to specify the result of an asynchronous connection attempt
ConnectionAttemptEvent - Class in com.impinj.octane
  This event carries information on a connection attempt.
ConnectionAttemptEvent() - Constructor for class com.impinj.octane.ConnectionAttemptEvent
ConnectionAttemptListener - Interface in com.impinj.octane
  Your application can implement this interface to receive connection attempt events.
ConnectionCloseEvent - Class in com.impinj.octane
  This event carries information on a connection close.
ConnectionCloseEvent() - Constructor for class com.impinj.octane.ConnectionCloseEvent
ConnectionCloseListener - Interface in com.impinj.octane
  Your application can implement this interface to receive connection close events.
ConnectionLostListener - Interface in com.impinj.octane
  Your application can implement this interface to receive connection close events.
contains(int) - Static method in enum com.impinj.octane.ReaderMode
  Deprecated.
crc - Static variable in class com.impinj.octane.BitPointers
  Constant used to point to the first bit of the CRC
Crc - Static variable in class com.impinj.octane.WordPointers
  The 1-word CRC is stored starting at this word in EPC memory

## D

Dbm - Variable in class com.impinj.octane.RxSensitivityTableEntry
  Receive sensitivity in dBm.
Dbm - Variable in class com.impinj.octane.TxPowerTableEntry
  Transmit power in dBm.
deleteAllOpSequences() - Method in class com.impinj.octane.ImpinjReader
  Deletes all tag operation sequences from the reader
deleteOpSequence(int) - Method in class com.impinj.octane.ImpinjReader
  Deletes a tag operation sequence
DiagnosticReport - Class in com.impinj.octane
  xArray diagnostic report
DiagnosticsReportListener - Interface in com.impinj.octane
  Your application can implement this interface to receive xarray diagnostic report events.
DirectionConfig - Class in com.impinj.octane
  A container that holds all of the configuration options for xArray's Direction feature.
DirectionConfig() - Constructor for class com.impinj.octane.DirectionConfig
  The default constructor, sets `DirectionMode` to `DirectionMode.HighPerformance` and the tag age interval to five seconds.
DirectionFieldOfView - Enum in com.impinj.octane
  Specified if a narrow or wide ring should be used when reading and tracking tag direction.
DirectionMode - Enum in com.impinj.octane
  Provides the options available for tweaking the xArray's operation when in direction mode.
DirectionReport - Class in com.impinj.octane
  DirectionReport that is received by implementors of `DirectionReportListener`, instantiated and populated by `ImpinjReader`
DirectionReportListener - Interface in com.impinj.octane
  Your application must implement this interface to receive direction reports.
DirectionReportType - Enum in com.impinj.octane
  DirectionReportType is an enum used to indicate the event that caused a `DirectionReport` to be sent.
DirectionTagPopulationStatus - Enum in com.impinj.octane
  Specifies the overflow status of a Direction Report
disableAll() - Method in class com.impinj.octane.AntennaConfigGroup
  Disable all antennas in the collection.
disableAll() - Method in class com.impinj.octane.GpiConfigGroup
  Disable all GPIs in the collection.
disableById(short[]) - Method in class com.impinj.octane.AntennaConfigGroup
  Disable antennas by providing a list of antenna IDs.
disableById(List<? extends Number>) - Method in class com.impinj.octane.AntennaConfigGroup
  Disable antennas by providing a list of antenna IDs.
disableByRing(short[]) - Method in class com.impinj.octane.AntennaConfigGroup
  Deprecated.
disableBySector(short[]) - Method in class com.impinj.octane.AntennaConfigGroup
  Deprecated.
disablePolarizedAntennas() - Method in class com.impinj.octane.AntennaConfigGroup
  Disable polarized antennas 1001-1052, 2001-2052
disconnect() - Method in class com.impinj.octane.ImpinjReader
  Disconnects the LLRP connection to the reader

## E

enableAll() - Method in class com.impinj.octane.AntennaConfigGroup
  Enable all antennas in the collection.
enableAll() - Method in class com.impinj.octane.GpiConfigGroup
  Enable all GPIs in the collection.
enableById(short[]) - Method in class com.impinj.octane.AntennaConfigGroup
  Enable antennas by providing a list of antenna IDs.
enableById(List<? extends Number>) - Method in class com.impinj.octane.AntennaConfigGroup
  Enable antennas by providing a list of antenna IDs.
enableByRing(short[]) - Method in class com.impinj.octane.AntennaConfigGroup
  Deprecated.
enableBySector(short[]) - Method in class com.impinj.octane.AntennaConfigGroup
  Deprecated.
enableOpSequence(int) - Method in class com.impinj.octane.ImpinjReader
  Enables the Tag Operation Sequence
enablePolarizedAntennas() - Method in class com.impinj.octane.AntennaConfigGroup
  Enable polarized antennas 1001-1052, 2001-2052
enableSector(short) - Method in class com.impinj.octane.DirectionConfig
  Adds the specified sector to the list of sectors that should be monitored for tag entrances, exits, and updates.
Epc - Static variable in class com.impinj.octane.BitPointers
  Constant used to point to the first bit of the EPC.
Epc - Static variable in class com.impinj.octane.WordPointers
  The variable length EPC is stored starting at this word in EPC memory
EpcLengthInWords(short) - Static method in class com.impinj.octane.PcBits
  Determine the EPC length (in words) from the PC bits
errorOccured(String) - Method in class com.impinj.octane.ImpinjReader

## F

FeatureSet - Class in com.impinj.octane
  The FeatureSet class holds the capabilities and features of an Impinj reader.
FeatureSet() - Constructor for class com.impinj.octane.FeatureSet
FeatureSet(GET_READER_CAPABILITIES_RESPONSE) - Constructor for class com.impinj.octane.FeatureSet
FilterSettings - Class in com.impinj.octane
  These filter settings describe the inventory filters applied by the reader.
FilterSettings() - Constructor for class com.impinj.octane.FilterSettings
fromBlockNumber(short) - Static method in class com.impinj.octane.BlockPermalockMask
  Creates a block permalock mask from the specified block.
fromBlockNumberArray(short[]) - Static method in class com.impinj.octane.BlockPermalockMask
  Creates a block permalock mask from an array of block numbers.
fromByteArray(byte[]) - Static method in class com.impinj.octane.TagData
  Creates a TagData object from an array of bytes
fromByteList(List<Byte>) - Static method in class com.impinj.octane.TagData
  Creates a TagData object from a List of bytes
fromDoubleWord(long) - Static method in class com.impinj.octane.TagData
  Creates a TagData object from a long integer
fromHexString(String) - Static method in class com.impinj.octane.TagData
  Creates a TagData object from a hexadecimal string
fromTID(String) - Static method in enum com.impinj.octane.TagModelName
  Convert a TID string to a tag model name object
fromWord(int) - Static method in class com.impinj.octane.TagData
  Creates a TagData object from an array of integers (words)
fromWordArray(int[]) - Static method in class com.impinj.octane.TagData
  Creates a TagData object from an array of integers (words)
fromWordList(List<Integer>) - Static method in class com.impinj.octane.TagData
  Creates a TagData object from a List of Integers

## G

get(int) - Method in class com.impinj.octane.GpiConfigGroup
get(int) - Method in class com.impinj.octane.GpoConfigGroup
get(String) - Method in class com.impinj.octane.RshellReply
  Gets the value of the rshell token with name key
get_sectorId() - Method in class com.impinj.octane.SectorConfig
get_txFrequenciesInMhz() - Method in class com.impinj.octane.SectorConfig
  This is only applicable in regions that allow frequency control
getAccessPassword() - Method in class com.impinj.octane.TagBlockPermalockOp
getAccessPassword() - Method in class com.impinj.octane.TagLockOp
getAccessPassword() - Method in class com.impinj.octane.TagMarginReadOp
getAccessPassword() - Method in class com.impinj.octane.TagQtGetOp
getAccessPassword() - Method in class com.impinj.octane.TagQtSetOp
getAccessPassword() - Method in class com.impinj.octane.TagReadOp
getAccessPassword() - Method in class com.impinj.octane.TagWriteOp
getAccessPasswordLockType() - Method in class com.impinj.octane.TagLockOp
getAccessRange() - Method in class com.impinj.octane.TagQtGetOpResult
getAccessRange() - Method in class com.impinj.octane.TagQtSetOp
getAccessSpec() - Method in class com.impinj.octane.ImpinjReader
  Get the Access Spec for checking reader configuration
getAddress() - Method in class com.impinj.octane.ImpinjReader
  Gest the IP address or hostname of the reader.
getAntenna(Number) - Method in class com.impinj.octane.AntennaConfigGroup
  Returns the antenna configuration for the specified antenna port.
getAntenna(short) - Method in class com.impinj.octane.AntennaStatusGroup
getAntennaChangeListener() - Method in class com.impinj.octane.ImpinjReader
getAntennaConfigs() - Method in class com.impinj.octane.AntennaConfigGroup
getAntennaCount() - Method in class com.impinj.octane.FeatureSet
getAntennaHub(short) - Method in class com.impinj.octane.AntennaHubStatusGroup
getAntennaHubList() - Method in class com.impinj.octane.AntennaHubStatusGroup
getAntennaHubStatusGroup() - Method in class com.impinj.octane.Status
getAntennaId() - Method in class com.impinj.octane.TagOpSequence
GetAntennaIdsByRing(List<? extends Number>, ReaderModel) - Static method in class com.impinj.octane.AntennaUtilities
  Accepts a list of rings and a reader model, and returns the list of antennas in the selected rings.
GetAntennaIdsBySector(List<? extends Number>, ReaderModel) - Static method in class com.impinj.octane.AntennaUtilities
  Accepts a list of sectors and a reader model, and returns the list of antennas in the selected sectors.
getAntennaList() - Method in class com.impinj.octane.AntennaStatusGroup
getAntennaPortNumber() - Method in class com.impinj.octane.Tag
getAntennas() - Method in class com.impinj.octane.Settings
getAntennaStatusGroup() - Method in class com.impinj.octane.Status
getAutoStart() - Method in class com.impinj.octane.Settings
getAutoStop() - Method in class com.impinj.octane.Settings
GetAvailableSectors(ReaderModel) - Static method in class com.impinj.octane.AntennaUtilities
  Gets the list of available sectors for the reader model.
getBitCount() - Method in class com.impinj.octane.TagFilter
getBitCount() - Method in class com.impinj.octane.TagSelectFilter
getBitLength() - Method in class com.impinj.octane.MarginReadMask
getBitPointer() - Method in class com.impinj.octane.TagFilter
getBitPointer() - Method in class com.impinj.octane.TagMarginReadOp
getBitPointer() - Method in class com.impinj.octane.TagSelectFilter
getBitPointer() - Method in class com.impinj.octane.TargetTag
getBitPointer() - Method in class com.impinj.octane.TruncatedReplySettings
  Select a starting bit location in the EPC memory bank that will be used for the truncating select command.
getBlockMask() - Method in class com.impinj.octane.TagBlockPermalockOp
getBlockWriteRetryCount() - Method in class com.impinj.octane.TagOpSequence
getBlockWriteWordCount() - Method in class com.impinj.octane.TagOpSequence
getBufferOverflowListener() - Method in class com.impinj.octane.ImpinjReader
getBufferWarningListener() - Method in class com.impinj.octane.ImpinjReader
getChannelInMhz() - Method in class com.impinj.octane.Tag
getComputeWindowSeconds() - Method in class com.impinj.octane.LocationConfig
  Compute Window the the smoothing window for averaging the location estimates.
getConfidenceFactors() - Method in class com.impinj.octane.LocationReport
getConnected() - Method in class com.impinj.octane.AntennaHubStatus
getConnectionAttemptListener() - Method in class com.impinj.octane.ImpinjReader
getConnectionCloseListener() - Method in class com.impinj.octane.ImpinjReader
getConnectionLostListener() - Method in class com.impinj.octane.ImpinjReader
getConnectTimeout() - Method in class com.impinj.octane.ImpinjReader
getCountBytes() - Method in class com.impinj.octane.TagData
  Returns the size of the tag data in bytes
getCrc() - Method in class com.impinj.octane.Tag
getData() - Method in class com.impinj.octane.LocationConfidenceFactors
getData() - Method in class com.impinj.octane.TagReadOpResult
getData() - Method in class com.impinj.octane.TagWriteOp
getData() - Method in class com.impinj.octane.TargetTag
getDataProfile() - Method in class com.impinj.octane.TagQtGetOpResult
getDataProfile() - Method in class com.impinj.octane.TagQtSetOp
getDebounceInMs() - Method in class com.impinj.octane.GpiConfig
getDiagnosticsReportedListener() - Method in class com.impinj.octane.ImpinjReader
getDirection() - Method in class com.impinj.octane.SpatialConfig
  Gets the reader's direction configuration.
getDirection() - Method in class com.impinj.octane.XArrayConfig
  Deprecated.
getDisabledAntennaList() - Method in class com.impinj.octane.LocationConfig
  Antennas can be disabled when configuring location.
getDurationInMs() - Method in class com.impinj.octane.AutoStopConfig
getEmptyFieldTimeoutInMs() - Method in class com.impinj.octane.LowDutyCycleSettings
  When the reader detects and empty field (no tags) for this time, on a given antenna, it will enter low duty cycle mode and check this antenna for tags only periodically.
getEnabled() - Method in class com.impinj.octane.KeepaliveConfig
getEnabledSectors() - Method in class com.impinj.octane.DirectionConfig
getEnableLinkMonitorMode() - Method in class com.impinj.octane.KeepaliveConfig
  In Link monitor mode, the reader will monitor keep alive responses from the SDk and close the connection if they are missed.
getEpc() - Method in class com.impinj.octane.DirectionReport
getEpc() - Method in class com.impinj.octane.LocationReport
getEpc() - Method in class com.impinj.octane.Tag
  Contains the contents of the tag EPC memory backscatter by the tag.
getEpcLengthInWords() - Method in class com.impinj.octane.TruncatedReplySettings
  The EPC length, in 16-bit words, of all tags in the field of view.
getEpcLockType() - Method in class com.impinj.octane.TagLockOp
getEpcSizeBits() - Method in class com.impinj.octane.TagModelDetails
getExecutionCount() - Method in class com.impinj.octane.TagOpSequence
getFacilityXLocationCm() - Method in class com.impinj.octane.PlacementConfig
  When operating multiple xArrays in a single facility, a common coordinate system is desirable across all xArrays so that location data can be interpreted store-wide.
getFacilityYLocationCm() - Method in class com.impinj.octane.PlacementConfig
  When operating multiple xArrays in a single facility, a common coordinate system is desirable across all xArrays so that location data can be interpreted store-wide.
getFault() - Method in class com.impinj.octane.AntennaHubStatus
getFieldOfView() - Method in class com.impinj.octane.DirectionConfig
getFieldPingIntervalInMs() - Method in class com.impinj.octane.LowDutyCycleSettings
  When in low duty cycle mode, the reader will check the field for tags on each antenna at least once every Ping Interval.
getFilterOp() - Method in class com.impinj.octane.TagFilter
getFilters() - Method in class com.impinj.octane.Settings
getFirmwareVersion() - Method in class com.impinj.octane.FeatureSet
getFirstDelayInMs() - Method in class com.impinj.octane.AutoStartConfig
  Not implemented
getFirstSeenSector() - Method in class com.impinj.octane.DirectionReport
getFirstSeenTime() - Method in class com.impinj.octane.DirectionReport
getFirstSeenTime() - Method in class com.impinj.octane.Tag
getGen2v2TagsOnly() - Method in class com.impinj.octane.TruncatedReplySettings
  If only Gen2v2 tags are in the field of view then setting the Gen2v2TagsOnly flag will perform an additional CRC check to further validate the integrity of the tag response.
getGpi(short) - Method in class com.impinj.octane.GpiConfigGroup
  Returns the settings for the specified GPI port.
getGpi(short) - Method in class com.impinj.octane.GpiStatusGroup
  Returns the status for the specified GPI port.
getGpiChangeListener() - Method in class com.impinj.octane.ImpinjReader
getGpiCount() - Method in class com.impinj.octane.FeatureSet
getGpiLevel() - Method in class com.impinj.octane.AutoStartConfig
getGpiLevel() - Method in class com.impinj.octane.AutoStopConfig
getGpiList() - Method in class com.impinj.octane.GpiStatusGroup
getGpiPortNumber() - Method in class com.impinj.octane.AutoStartConfig
getGpiPortNumber() - Method in class com.impinj.octane.AutoStopConfig
getGpis() - Method in class com.impinj.octane.Settings
getGpiStatusGroup() - Method in class com.impinj.octane.Status
getGpo(short) - Method in class com.impinj.octane.GpoConfigGroup
  eturns the settings for the specified GPO port.
getGpoCount() - Method in class com.impinj.octane.FeatureSet
getGpoPulseDurationMsec() - Method in class com.impinj.octane.GpoConfig
getGpos() - Method in class com.impinj.octane.Settings
getGpsCoodinates() - Method in class com.impinj.octane.Tag
getHeightCm() - Method in class com.impinj.octane.PlacementConfig
  The xArray needs to know its height above ground level to perform location calculations.
getHoldReportsOnDisconnect() - Method in class com.impinj.octane.Settings
  When the reader is running an inventory it may be collecting tag reports.
getHubId() - Method in class com.impinj.octane.AntennaHubStatus
getId() - Method in class com.impinj.octane.TagOpSequence
getIncludeAntennaPortNumber() - Method in class com.impinj.octane.ReportConfig
getIncludeChannel() - Method in class com.impinj.octane.ReportConfig
getIncludeCrc() - Method in class com.impinj.octane.ReportConfig
getIncludeDopplerFrequency() - Method in class com.impinj.octane.ReportConfig
getIncludeFastId() - Method in class com.impinj.octane.ReportConfig
getIncludeFirstSeenTime() - Method in class com.impinj.octane.ReportConfig
getIncludeGpsCoordinates() - Method in class com.impinj.octane.ReportConfig
getIncludeLastSeenTime() - Method in class com.impinj.octane.ReportConfig
getIncludePcBits() - Method in class com.impinj.octane.ReportConfig
getIncludePeakRssi() - Method in class com.impinj.octane.ReportConfig
getIncludePhaseAngle() - Method in class com.impinj.octane.ReportConfig
getIncludeSeenCount() - Method in class com.impinj.octane.ReportConfig
getIsConnected() - Method in class com.impinj.octane.Status
getIsEnabled() - Method in class com.impinj.octane.GpiConfig
getIsEnabled() - Method in class com.impinj.octane.LowDutyCycleSettings
getIsEnabled() - Method in class com.impinj.octane.TruncatedReplySettings
  Get flag indicating whether the Truncated Reply feature is enabled.
getIsMaxRxSensitivity() - Method in class com.impinj.octane.AntennaConfig
  Typically an antenna is set to maximum sensitivity.
getIsMaxRxSensitivity() - Method in class com.impinj.octane.AntennaConfigGroup
getIsMaxTxPower() - Method in class com.impinj.octane.AntennaConfig
  Typically an antenna is set to maximum transmit power.
getIsMaxTxPower() - Method in class com.impinj.octane.AntennaConfigGroup
getIsMaxTxPower() - Method in class com.impinj.octane.DirectionConfig
getIsMaxTxPower() - Method in class com.impinj.octane.LocationConfig
  Typically an antenna is set to maximum transmit power.
getIsSingulating() - Method in class com.impinj.octane.Status
getKeepaliveListener() - Method in class com.impinj.octane.ImpinjReader
getKeepalives() - Method in class com.impinj.octane.Settings
getKillPassword() - Method in class com.impinj.octane.TagKillOp
getKillPasswordLockType() - Method in class com.impinj.octane.TagLockOp
getLastReadSector() - Method in class com.impinj.octane.DirectionReport
getLastReadTime() - Method in class com.impinj.octane.DirectionReport
getLastSeenTime() - Method in class com.impinj.octane.Tag
getLatitude() - Method in class com.impinj.octane.GpsCoordinates
getLinkDownThreshold() - Method in class com.impinj.octane.KeepaliveConfig
  In Link monitoring mode, this setting determines how many keep alives can be missed before the connection closes.
getLocalDateTime() - Method in class com.impinj.octane.ImpinjTimestamp
  Utility that outputs the ImpinjTimestamp data in local time format.
getLocation() - Method in class com.impinj.octane.SpatialConfig
  Gets the reader's location configuration.
getLocation() - Method in class com.impinj.octane.XArrayConfig
  Deprecated.
getLocationAlgorithmControlList() - Method in class com.impinj.octane.LocationConfig
  Custom location algorithm control parameters can be set when configuring location.
getLocationReportedListener() - Method in class com.impinj.octane.ImpinjReader
getLocationXCm() - Method in class com.impinj.octane.LocationReport
getLocationYCm() - Method in class com.impinj.octane.LocationReport
getLockCount() - Method in class com.impinj.octane.TagLockOp
getLockResult() - Method in class com.impinj.octane.LockTagResult
getLongitude() - Method in class com.impinj.octane.GpsCoordinates
getLowDutyCycle() - Method in class com.impinj.octane.Settings
getMarginMask() - Method in class com.impinj.octane.TagMarginReadOp
getMask() - Method in class com.impinj.octane.BlockPermalockMask
getMask() - Method in class com.impinj.octane.MarginReadMask
getMask() - Method in class com.impinj.octane.TargetTag
getMatchingAction() - Method in class com.impinj.octane.TagSelectFilter
getMaxNumSelectFiltersPerQuery() - Method in class com.impinj.octane.FeatureSet
getMaxOperationSequences() - Method in class com.impinj.octane.FeatureSet
getMaxOperationsPerSequence() - Method in class com.impinj.octane.FeatureSet
getMaxTxPower() - Method in class com.impinj.octane.SectorConfig
getMemoryBank() - Method in class com.impinj.octane.TagFilter
getMemoryBank() - Method in class com.impinj.octane.TagMarginReadOp
getMemoryBank() - Method in class com.impinj.octane.TagReadOp
getMemoryBank() - Method in class com.impinj.octane.TagSelectFilter
getMemoryBank() - Method in class com.impinj.octane.TagWriteOp
getMemoryBank() - Method in class com.impinj.octane.TargetTag
getMessageTimeout() - Method in class com.impinj.octane.ImpinjReader
getMetrics() - Method in class com.impinj.octane.DiagnosticReport
getMode() - Method in class com.impinj.octane.AutoStartConfig
getMode() - Method in class com.impinj.octane.AutoStopConfig
getMode() - Method in class com.impinj.octane.DirectionConfig
getMode() - Method in class com.impinj.octane.FilterSettings
getMode() - Method in class com.impinj.octane.GpoConfig
getMode() - Method in class com.impinj.octane.ReportConfig
  The report Mode specifies when tag reports are generated
getMode() - Method in class com.impinj.octane.SpatialConfig
  Tracks the mode (Inventory, Location, or Direction) the reader with location or direction role capabilities is currently in.
getMode() - Method in class com.impinj.octane.XArrayConfig
  Deprecated.
getModelDetails() - Method in class com.impinj.octane.Tag
getModelName() - Method in class com.impinj.octane.FeatureSet
getModelName() - Method in class com.impinj.octane.TagModelDetails
getModelNumber() - Method in class com.impinj.octane.FeatureSet
getName() - Method in class com.impinj.octane.ImpinjReader
  Gets the name assigned to a reader
getNonMatchingAction() - Method in class com.impinj.octane.TagSelectFilter
getNumWordsWritten() - Method in class com.impinj.octane.TagWriteOpResult
getOpId() - Method in class com.impinj.octane.TagOpResult
getOps() - Method in class com.impinj.octane.TagOpSequence
GetOptimizedAntennaList(ReaderModel) - Static method in class com.impinj.octane.AntennaUtilities
  Get the optimized antenna list for the provided reader model.
getOptimizedReadOps() - Method in class com.impinj.octane.ReportConfig
  When optimized reads are enabled, the report can contain optimized read reports.
getOrientationDegrees() - Method in class com.impinj.octane.PlacementConfig
  When operating multiple xArrays in a single facility, a common coordinate system is desirable across all xArrays so that location data can be interpreted store-wide.
getPcBits() - Method in class com.impinj.octane.Tag
getPeakRssiInDbm() - Method in class com.impinj.octane.Tag
getPercentFull() - Method in class com.impinj.octane.BufferWarningEvent
getPeriodInMs() - Method in class com.impinj.octane.AutoStartConfig
  When using the periodic autostart trigger, the reader will initiate inventory periodically.
getPeriodInMs() - Method in class com.impinj.octane.KeepaliveConfig
getPersistence() - Method in class com.impinj.octane.TagQtSetOp
getPhaseAngleInRadians() - Method in class com.impinj.octane.Tag
getPlacement() - Method in class com.impinj.octane.SpatialConfig
  Gets the reader's placement configuration.
getPlacement() - Method in class com.impinj.octane.XArrayConfig
  Deprecated.
getPolarizationEnabled() - Method in class com.impinj.octane.AntennaConfigGroup
getPortName() - Method in class com.impinj.octane.AntennaConfig
  For convenience the antenna configuration hold a user defined port name.
getPortNumber() - Method in class com.impinj.octane.AntennaConfig
  Each antenna is identified by the port number
getPortNumber() - Method in class com.impinj.octane.AntennaEvent
getPortNumber() - Method in class com.impinj.octane.AntennaStatus
getPortNumber() - Method in class com.impinj.octane.GpiConfig
getPortNumber() - Method in class com.impinj.octane.GpiEvent
getPortNumber() - Method in class com.impinj.octane.GpiStatus
getPortNumber() - Method in class com.impinj.octane.GpoConfig
getReadCount() - Method in class com.impinj.octane.LocationConfidenceFactors
getReaderMode() - Method in class com.impinj.octane.Settings
  Deprecated.
  The `ReaderMode` enum is no longer supported.

  Use `Settings.getRfMode()` instead. ReaderMode is the preselected set of gen2 physical layer settings to optimize tag communications for a certain scenario and environment

getReaderModel() - Method in class com.impinj.octane.FeatureSet
getReaderModes() - Method in class com.impinj.octane.FeatureSet
  Deprecated.
  The `ReaderMode` enum is no longer supported.

  Use `FeatureSet.getRfModes()` instead.

getReaderStartListener() - Method in class com.impinj.octane.ImpinjReader
getReaderStopListener() - Method in class com.impinj.octane.ImpinjReader
getReadOperationResults() - Method in class com.impinj.octane.Tag
getReducedPowerFrequenciesInMhz() - Method in class com.impinj.octane.Settings
getReport() - Method in class com.impinj.octane.Settings
getReportType() - Method in class com.impinj.octane.DirectionReport
getReportType() - Method in class com.impinj.octane.LocationReport
getResult() - Method in class com.impinj.octane.TagBlockPermalockOpResult
getResult() - Method in class com.impinj.octane.TagKillOpResult
getResult() - Method in class com.impinj.octane.TagLockOpResult
getResult() - Method in class com.impinj.octane.TagMarginReadOpResult
getResult() - Method in class com.impinj.octane.TagQtGetOpResult
getResult() - Method in class com.impinj.octane.TagQtSetOpResult
getResult() - Method in class com.impinj.octane.TagReadOpResult
getResult() - Method in class com.impinj.octane.TagWriteOpResult
getResults() - Method in class com.impinj.octane.TagOpReport
getRfDopplerFrequency() - Method in class com.impinj.octane.Tag
getRfMode() - Method in class com.impinj.octane.Settings
  RfMode is the preselected set of gen2 physical layer settings to optimize tag communications for a certain scenario and environment
getRfModes() - Method in class com.impinj.octane.FeatureSet
getRxSensitivities() - Method in class com.impinj.octane.FeatureSet
getRxSensitivityinDbm() - Method in class com.impinj.octane.AntennaConfig
  Receive Sensitivity can be adjusted on the antenna to prevent the reader from receiving weak responses from tags.
getRxSensitivityinDbm() - Method in class com.impinj.octane.AntennaConfigGroup
getRxSensitivityInDbm() - Method in class com.impinj.octane.SectorConfig
getSearchMode() - Method in class com.impinj.octane.Settings
  Gen2 provides rudimentary building blocks to inventory populations of tags The Impinj reader creates high level inventory search modes from these gen2 operations.
getSequenceId() - Method in class com.impinj.octane.TagOpResult
getSequenceStopTrigger() - Method in class com.impinj.octane.TagOpSequence
getSerialNumber() - Method in class com.impinj.octane.FeatureSet
getSession() - Method in class com.impinj.octane.Settings
  Sets the gen2 session for the reader.
getSpatialConfig() - Method in class com.impinj.octane.Settings
  Gets the reader settings object that contains configurations specific to readers with location and direction role capabilities.
getState() - Method in class com.impinj.octane.AntennaEvent
getState() - Method in class com.impinj.octane.TagOpSequence
getTag() - Method in class com.impinj.octane.TagOpResult
getTagAgeIntervalSeconds() - Method in class com.impinj.octane.DirectionConfig
  The "age interval" specifies how long a tag needs to go unseen before it's removed from the population of tags tracked for direction and an exit report is sent.
getTagAgeIntervalSeconds() - Method in class com.impinj.octane.LocationConfig
  The Age Interval specifies how long a tag needs to go unseen before its removed from the location tracking.
getTagFilter1() - Method in class com.impinj.octane.FilterSettings
getTagFilter2() - Method in class com.impinj.octane.FilterSettings
getTagMask() - Method in class com.impinj.octane.TagFilter
getTagMask() - Method in class com.impinj.octane.TagSelectFilter
getTagMask() - Method in class com.impinj.octane.TruncatedReplySettings
  Specifies the mask that must match the EPC memory bank starting at Pointer.
getTagOpCompleteListener() - Method in class com.impinj.octane.ImpinjReader
getTagPopulationEstimate() - Method in class com.impinj.octane.Settings
  When performing inventory operations, the Impinj reader uses the gen2 protocol's random access method to arbitrate between populations of tags.
getTagPopulationStatus() - Method in class com.impinj.octane.DirectionReport
getTagReportListener() - Method in class com.impinj.octane.ImpinjReader
getTags() - Method in class com.impinj.octane.TagReport
getTagSeenCount() - Method in class com.impinj.octane.Tag
getTagSelectFilterList() - Method in class com.impinj.octane.FilterSettings
  Get the tag select filter list, which is the new interface for setting tag filter behavior.
getTargetTag() - Method in class com.impinj.octane.TagOpSequence
getTemperatureCelsius() - Method in class com.impinj.octane.Status
getTid() - Method in class com.impinj.octane.Tag
getTidLockType() - Method in class com.impinj.octane.TagLockOp
getTiltSensorValue() - Method in class com.impinj.octane.Status
getTimeout() - Method in class com.impinj.octane.AutoStopConfig
getTimestamp() - Method in class com.impinj.octane.LocationReport
getTruncatedReply() - Method in class com.impinj.octane.Settings
getTxFrequencies() - Method in class com.impinj.octane.FeatureSet
getTxFrequenciesInMhz() - Method in class com.impinj.octane.Settings
getTxPowerinDbm() - Method in class com.impinj.octane.AntennaConfig
  Transmit power can be adjusted on the antenna to reduce the read range of the antenna.
getTxPowerinDbm() - Method in class com.impinj.octane.AntennaConfigGroup
getTxPowerinDbm() - Method in class com.impinj.octane.DirectionConfig
getTxPowerinDbm() - Method in class com.impinj.octane.LocationConfig
  Transmit power can be adjusted on antennas to reduce the read range of the antenna.
getTxPowerInDbm() - Method in class com.impinj.octane.SectorConfig
getTxPowers() - Method in class com.impinj.octane.FeatureSet
getUpdateIntervalSeconds() - Method in class com.impinj.octane.DirectionConfig
  Specifies how often update reports are sent when updates are enabled.
getUpdateIntervalSeconds() - Method in class com.impinj.octane.LocationConfig
  The UpdateInterval specifies how often tag reports are generated when tag report updates are enabled
getUserLockType() - Method in class com.impinj.octane.TagLockOp
getUserMemorySizeBits() - Method in class com.impinj.octane.TagModelDetails
getUserTagPopulationLimit() - Method in class com.impinj.octane.DirectionConfig
getUtcTimestamp() - Method in class com.impinj.octane.AutoStartConfig
  TODO
getUtcTimestamp() - Method in class com.impinj.octane.ImpinjTimestamp
getValue() - Method in enum com.impinj.octane.AntennaEventType
getValue() - Method in enum com.impinj.octane.AutoStartMode
getValue() - Method in enum com.impinj.octane.AutoStopMode
getValue() - Method in enum com.impinj.octane.BlockPermalockResult
getValue() - Method in enum com.impinj.octane.GpoMode
getValue() - Method in enum com.impinj.octane.HubConnectedStatus
getValue() - Method in enum com.impinj.octane.HubFaultStatus
getValue() - Method in enum com.impinj.octane.KillResultStatus
getValue() - Method in enum com.impinj.octane.LocationReportType
getValue() - Method in enum com.impinj.octane.LockMemoryBank
getValue() - Method in enum com.impinj.octane.LockResultStatus
getValue() - Method in enum com.impinj.octane.LockType
getValue() - Method in enum com.impinj.octane.MarginReadResult
getValue() - Method in enum com.impinj.octane.MemoryBank
getValue() - Method in enum com.impinj.octane.QtAccessRange
getValue() - Method in enum com.impinj.octane.QtDataProfile
getValue() - Method in enum com.impinj.octane.QtGetConfigResultStatus
getValue() - Method in enum com.impinj.octane.QtPersistence
getValue() - Method in enum com.impinj.octane.QtSetConfigResultStatus
getValue() - Method in enum com.impinj.octane.ReaderMode
  Deprecated.
getValue() - Method in enum com.impinj.octane.ReaderModel
getValue() - Method in enum com.impinj.octane.ReadResultStatus
getValue() - Method in enum com.impinj.octane.ReportMode
getValue() - Method in enum com.impinj.octane.SearchMode
getValue() - Method in enum com.impinj.octane.SequenceState
getValue() - Method in enum com.impinj.octane.SequenceTriggerType
getValue() - Method in enum com.impinj.octane.TagFilterMode
getValue() - Method in enum com.impinj.octane.TagLockState
getValue() - Method in enum com.impinj.octane.WriteResultStatus
getWordCount() - Method in class com.impinj.octane.TagReadOp
getWordPointer() - Method in class com.impinj.octane.TagReadOp
getWordPointer() - Method in class com.impinj.octane.TagWriteOp
getXArray() - Method in class com.impinj.octane.Settings
  Deprecated.
getxAxis() - Method in class com.impinj.octane.TiltSensorValue
getyAxis() - Method in class com.impinj.octane.TiltSensorValue
GpiChangeListener - Interface in com.impinj.octane
  Your application can implement this interface to receive GPI change events.
GpiConfig - Class in com.impinj.octane
  This class holds the configuration for a single General Purpose Input
GpiConfig() - Constructor for class com.impinj.octane.GpiConfig
GpiConfigGroup - Class in com.impinj.octane
  Hold the configuration for a collection of General Purpose Inputs
GpiEvent - Class in com.impinj.octane
  Class used to encapsulate the details of a GPI change reader event.
GpiEvent() - Constructor for class com.impinj.octane.GpiEvent
GpiStatus - Class in com.impinj.octane
  Contains the information on the status of a single GPI
GpiStatus() - Constructor for class com.impinj.octane.GpiStatus
GpiStatusGroup - Class in com.impinj.octane
  Container class encapsulating all of the GPI status objects.
GpoConfig - Class in com.impinj.octane
  Container class for holding the configuration of a single General Purpose output
GpoConfig() - Constructor for class com.impinj.octane.GpoConfig
GpoConfigGroup - Class in com.impinj.octane
  Container class for holding the General Purpose Output (GPO) configuration for the readers set of output
GpoMode - Enum in com.impinj.octane
  An enumeration that holds the possible GPO configuration values.
GpsCoordinates - Class in com.impinj.octane
  A container class to hold latitude and longitude information
GpsCoordinates() - Constructor for class com.impinj.octane.GpsCoordinates

## H

HubConnectedStatus - Enum in com.impinj.octane
  Container class to hold Impinj Antenna Hub Information
HubFaultStatus - Enum in com.impinj.octane
  Container class to hold antenna hub fault information

## I

Id - Variable in class com.impinj.octane.TagOp
ImpinjReader - Class in com.impinj.octane
  This is the main class for the Octane SDK Java.
ImpinjReader(String, String, int) - Constructor for class com.impinj.octane.ImpinjReader
  Creates and initializes an ImpinjReader object.
ImpinjReader(String, String) - Constructor for class com.impinj.octane.ImpinjReader
  Creates and initializes an ImpinjReader object.
ImpinjReader() - Constructor for class com.impinj.octane.ImpinjReader
  Creates and initializes an ImpinjReader object.
ImpinjReader.MessageHandler - Class in com.impinj.octane
ImpinjTimestamp - Class in com.impinj.octane
  Timestamp class supporting Impinj Reader and LLRP timestamp data.
ImpinjTimestamp() - Constructor for class com.impinj.octane.ImpinjTimestamp
  Default constructor.
ImpinjTimestamp(Date) - Constructor for class com.impinj.octane.ImpinjTimestamp
  Constructor that translates standard DateTime data into ImpinjTimeStamp format.
ImpinjTimestamp(long) - Constructor for class com.impinj.octane.ImpinjTimestamp
  Constructor that takes unsigned long (Impinj reader) timestamp data.
ImpinjTimestamp(Timestamp) - Constructor for class com.impinj.octane.ImpinjTimestamp
  Constructor that takes LLRP timestamp data.
Index - Variable in class com.impinj.octane.RxSensitivityTableEntry
  Reader internal receiver sensitivity table index.
Index - Variable in class com.impinj.octane.TxPowerTableEntry
  Reader internal transmit power table index.
intValue() - Method in enum com.impinj.octane.CommunicationsStandardType
  Converts the enumeration object to an integer value
isAntennaPortNumberPresent() - Method in class com.impinj.octane.Tag
isBlockWrite() - Method in class com.impinj.octane.TagWriteOpResult
isBlockWriteEnabled() - Method in class com.impinj.octane.TagOpSequence
isChannelInMhzPresent() - Method in class com.impinj.octane.Tag
isConnected() - Method in class com.impinj.octane.AntennaStatus
isConnected() - Method in class com.impinj.octane.ImpinjReader
isConnected() - Method in interface com.impinj.octane.RShellSocket
isConnected() - Method in class com.impinj.octane.SshRShellSocket
isConnected() - Method in class com.impinj.octane.TelnetRShellSocket
isCrcPresent() - Method in class com.impinj.octane.Tag
isDiagnosticReportEnabled() - Method in class com.impinj.octane.DirectionConfig
  When enabled, diagnostic reports are generated at each update interval and sent to the application
isDiagnosticReportEnabled() - Method in class com.impinj.octane.LocationConfig
  When enabled, diagnostic reports are generated at each update interval and sent to the application
isEnabled() - Method in class com.impinj.octane.AntennaConfig
  An antenna can be enabled or disabled.
isEntryReportEnabled() - Method in class com.impinj.octane.DirectionConfig
  When enabled, an entry report is sent immediately upon the tag entering the field of view of the reader.
isEntryReportEnabled() - Method in class com.impinj.octane.LocationConfig
  When enabled, an entry report is sent immediately upon the tag entering the field of view of the reader.
isExitReportEnabled() - Method in class com.impinj.octane.DirectionConfig
  When enabled, an exit report is generated when the tag has not been seen by the reader in the tag age Interval.
isExitReportEnabled() - Method in class com.impinj.octane.LocationConfig
  When enabled, an exit report is generated when the tag has not been seen by the reader in the tag age Interval.
isFastIdAvailable() - Method in class com.impinj.octane.FeatureSet
isFastIdPresent() - Method in class com.impinj.octane.Tag
isFilteringAvailable() - Method in class com.impinj.octane.FeatureSet
isFirstSeenTimePresent() - Method in class com.impinj.octane.Tag
isGpiDebounceAvailable() - Method in class com.impinj.octane.FeatureSet
isGpsCoordinatesPresent() - Method in class com.impinj.octane.Tag
isHoppingRegion() - Method in class com.impinj.octane.FeatureSet
isImpinjRssiReportingAvailable() - Method in class com.impinj.octane.FeatureSet
isLastSeenTimePresent() - Method in class com.impinj.octane.Tag
isLinkMonitorAvailable() - Method in class com.impinj.octane.FeatureSet
isMaxRxSensitivity() - Method in class com.impinj.octane.SectorConfig
isMultiwordBlockWriteAvailable() - Method in class com.impinj.octane.FeatureSet
isPcBitsPresent() - Method in class com.impinj.octane.Tag
isPeakRssiInDbmPresent() - Method in class com.impinj.octane.Tag
isPhaseAngleReportingAvailable() - Method in class com.impinj.octane.FeatureSet
isQueueEmpty() - Method in class com.impinj.octane.BackgroundWorker
isRfDopplerFrequencyPresent() - Method in class com.impinj.octane.Tag
isRfPhaseAnglePresent() - Method in class com.impinj.octane.Tag
isSectorConfigurationValid() - Method in class com.impinj.octane.DirectionConfig
  Deprecated.
isSectorEnabled(short) - Method in class com.impinj.octane.DirectionConfig
  Tests if the specified sector is in the list of sectors that should be monitored for tag entrances, exits, and updates.
isSeenCountPresent() - Method in class com.impinj.octane.Tag
isSpatialReader() - Method in class com.impinj.octane.ImpinjReader
  Detects if the connected reader is a reader with direction or location role capabilities (xArray or xSpan).
isSpatialReader() - Method in enum com.impinj.octane.ReaderModel
  Detects if the connected reader is a reader with direction or location role capabilities (xArray or xSpan).
isState() - Method in class com.impinj.octane.GpiEvent
isState() - Method in class com.impinj.octane.GpiStatus
isSupportsQt() - Method in class com.impinj.octane.TagModelDetails
isTagAccessAvailable() - Method in class com.impinj.octane.FeatureSet
isTryingToStop() - Method in class com.impinj.octane.BackgroundWorker
isUpdateReportEnabled() - Method in class com.impinj.octane.DirectionConfig
  When update reports are enabled, direction reports are sent by the reader periodically for all tags in the direction database
isUpdateReportEnabled() - Method in class com.impinj.octane.LocationConfig
  When update reports are enabled, location reports are sent by the reader periodically for all tags in the location database
isXArray() - Method in class com.impinj.octane.ImpinjReader
  Detects if the connected reader is an xArray.
isXArray() - Method in enum com.impinj.octane.ReaderModel
  Detects if the connected reader is an xArray.
isXSpan() - Method in class com.impinj.octane.ImpinjReader
  Detects if the connected reader is an xSpan.
iterator() - Method in class com.impinj.octane.AntennaConfigGroup
  provides an interator to traverse the list of antenna configurations
iterator() - Method in class com.impinj.octane.GpiConfigGroup
iterator() - Method in class com.impinj.octane.GpoConfigGroup

## K

KeepaliveConfig - Class in com.impinj.octane
  A class to hold the settings of the keepalive feature
KeepaliveConfig() - Constructor for class com.impinj.octane.KeepaliveConfig
KeepaliveEvent - Class in com.impinj.octane
  This event carries information on a keepalive event.
KeepaliveEvent() - Constructor for class com.impinj.octane.KeepaliveEvent
KeepaliveListener - Interface in com.impinj.octane
  Your application can implement this interface to receive keepalive events.
KeepaliveTimeoutListener - Interface in com.impinj.octane
  An internal class used by the SDK to watch for keepalive timeouts
KeepaliveTimer - Class in com.impinj.octane
  An internal class that watches the keep alive messages from the reader
KeepaliveTimer() - Constructor for class com.impinj.octane.KeepaliveTimer
KillPassword - Static variable in class com.impinj.octane.WordPointers
  The 2-word kill password is stored at this word in reserved memory
KillResultStatus - Enum in com.impinj.octane
  An enumeration that describes the result of a kill tag operation

## L

load(String) - Static method in class com.impinj.octane.FeatureSet
  Read the representation of FeatureSet from a file and return a new FeatureSet instance with those values.
load(String) - Static method in class com.impinj.octane.Settings
  builds a settings object from a file (from save)
LocationConfidenceFactors - Class in com.impinj.octane
  Contains the confidence factors for a location report.
LocationConfig - Class in com.impinj.octane
  A container that holds all of the configuration options for xArray location
LocationConfig() - Constructor for class com.impinj.octane.LocationConfig
LocationReport - Class in com.impinj.octane
  xArray location report.
LocationReportListener - Interface in com.impinj.octane
  Your application can implement this interface to receive location reports.
LocationReportType - Enum in com.impinj.octane
  The type of the location report generated by the reader.
LockMemoryBank - Enum in com.impinj.octane
  An enumeration describing which memory bank to lock
LockResultStatus - Enum in com.impinj.octane
  The status of a lock operation
LockTagResult - Class in com.impinj.octane
  Class to carry the result of a lock operation
LockTagResult() - Constructor for class com.impinj.octane.LockTagResult
LockType - Enum in com.impinj.octane
  An enumeration that holds the type of lock operation to perform
LowDutyCycleSettings - Class in com.impinj.octane
  The Impinj reader can operation automatically in a low duty cycle mode, performing continuous inventory when tags are present, but reducing the duty cycle of the inventory when tags have been absent from the field for some time.
LowDutyCycleSettings() - Constructor for class com.impinj.octane.LowDutyCycleSettings

## M

MarginReadMask - Class in com.impinj.octane
  Used to specify the mask to margin read
MarginReadMask() - Constructor for class com.impinj.octane.MarginReadMask
  Constructor for MarginReadMask initializes empty defaults.
MarginReadResult - Enum in com.impinj.octane
  An enumeration to hold the margin read result.
MemoryBank - Enum in com.impinj.octane
  Gen2 defines several memory banks.
messageReceived(LLRPMessage) - Method in class com.impinj.octane.ImpinjReader
  For internal use only to receive messages from the LLRP library

## O

OctaneSdkException - Exception in com.impinj.octane
  When errors occur in the SDK, this exception is thrown.
OctaneSdkException(String) - Constructor for exception com.impinj.octane.OctaneSdkException
onAntennaChanged(ImpinjReader, AntennaEvent) - Method in interface com.impinj.octane.AntennaChangeListener
onBufferOverflow(ImpinjReader, BufferOverflowEvent) - Method in interface com.impinj.octane.BufferOverflowListener
onBufferWarning(ImpinjReader, BufferWarningEvent) - Method in interface com.impinj.octane.BufferWarningListener
onConnectionAttempt(ImpinjReader, ConnectionAttemptEvent) - Method in interface com.impinj.octane.ConnectionAttemptListener
onConnectionClose(ImpinjReader, ConnectionCloseEvent) - Method in interface com.impinj.octane.ConnectionCloseListener
onConnectionLost(ImpinjReader) - Method in interface com.impinj.octane.ConnectionLostListener
onDiagnosticsReported(ImpinjReader, DiagnosticReport) - Method in interface com.impinj.octane.DiagnosticsReportListener
onDirectionReported(ImpinjReader, DirectionReport) - Method in interface com.impinj.octane.DirectionReportListener
onGpiChanged(ImpinjReader, GpiEvent) - Method in interface com.impinj.octane.GpiChangeListener
onKeepalive(ImpinjReader, KeepaliveEvent) - Method in interface com.impinj.octane.KeepaliveListener
onKeepaliveTimeout() - Method in class com.impinj.octane.ImpinjReader
onKeepaliveTimeout() - Method in interface com.impinj.octane.KeepaliveTimeoutListener
onLocationReported(ImpinjReader, LocationReport) - Method in interface com.impinj.octane.LocationReportListener
onReaderStart(ImpinjReader, ReaderStartEvent) - Method in interface com.impinj.octane.ReaderStartListener
onReaderStop(ImpinjReader, ReaderStopEvent) - Method in interface com.impinj.octane.ReaderStopListener
onTagOpComplete(ImpinjReader, TagOpReport) - Method in interface com.impinj.octane.TagOpCompleteListener
onTagReported(ImpinjReader, TagReport) - Method in interface com.impinj.octane.TagReportListener
open(String, String, String, int, RShellConnectionType) - Method in class com.impinj.octane.RshellEngine
  Used to open an RShell session with the Impinj reader.
open(String, String, String, int) - Method in class com.impinj.octane.RshellEngine
  Deprecated.
  Telnet has been deprecated. Use OpenSecureSession() instead.
openSecureSession(String, String, String, int) - Method in class com.impinj.octane.RshellEngine
  Used to open a secure SSH RShell session with the Impinj reader.

## P

pc - Static variable in class com.impinj.octane.BitPointers
  Constant used to point to the first bit of the Protocol Control Bits
PcBits - Class in com.impinj.octane
  Helper class used to encode and decode the PC word.
PcBits() - Constructor for class com.impinj.octane.PcBits
PcBits - Static variable in class com.impinj.octane.WordPointers
  The 1-word PCBits are stored starting that this word in EPC memory
PlacementConfig - Class in com.impinj.octane
  Since xArray reports location, it requires knowledge of its exact placement, especially when there are multiple xArrays reporting location and the user requires a consistent coordinate system.
PlacementConfig() - Constructor for class com.impinj.octane.PlacementConfig

## Q

QtAccessRange - Enum in com.impinj.octane
  Enumeration used to determine whether to configure the tag in reduced sensitivity (i.e.
QtDataProfile - Enum in com.impinj.octane
  Enumeration used to determine which QT data profile to use.
QtGetConfigResultStatus - Enum in com.impinj.octane
  An enumeration to describe the result of a QT Get Command operation
QtPersistence - Enum in com.impinj.octane
  Enumeration used to determine whether the QT set command should persist
QtSetConfigResultStatus - Enum in com.impinj.octane
  An enumeration to describe the result of a QT Set Command operation
queryDefaultSettings() - Method in class com.impinj.octane.ImpinjReader
  Queries the default settings of the reader.
queryFeatureSet() - Method in class com.impinj.octane.ImpinjReader
  Queries the reader for a summary of the features that it supports.
querySettings() - Method in class com.impinj.octane.ImpinjReader
  This function queries the reader for its current settings.
queryStatus() - Method in class com.impinj.octane.ImpinjReader
  queries status information from the reader
queryTags() - Method in class com.impinj.octane.ImpinjReader
  Tells the reader to send all the tag reports it has buffered.

## R

readerIsXArray() - Method in class com.impinj.octane.ImpinjReader
  Deprecated.
ReaderMode - Enum in com.impinj.octane
  Deprecated.
  The `ReaderMode` enum is no longer supported.

  Use `Settings.setRfMode(Integer)` and `Settings.getRfMode()` to set the RF Mode instead. An enumeration defining the choices for the communications parameters used between the reader and tags. These are pre-selected and tested values for Tari, M, TR etc which have been optimized for the best performance with Impinj readers.

ReaderModel - Enum in com.impinj.octane
  All the possible reader models, mapped to their model numbers.
ReaderStartEvent - Class in com.impinj.octane
  This event carries information on a reader start event.
ReaderStartEvent() - Constructor for class com.impinj.octane.ReaderStartEvent
ReaderStartListener - Interface in com.impinj.octane
  Your application can implement this interface to receive reader start events.
ReaderStopEvent - Class in com.impinj.octane
  This event carries information on a reader stop event.
ReaderStopEvent() - Constructor for class com.impinj.octane.ReaderStopEvent
ReaderStopListener - Interface in com.impinj.octane
  Your application can implement this interface to receive reader stop events.
ReadResultStatus - Enum in com.impinj.octane
  An enumeration that conveys the status of a tag read operation
removeAllSectors() - Method in class com.impinj.octane.DirectionConfig
  Removes all sectors from the list of sectors that should be monitored for tag entrances, exits, and updates.
removeAntennaChangeListener() - Method in class com.impinj.octane.ImpinjReader
  Removes the antenna change listener.
removeDiagnosticsReportListener() - Method in class com.impinj.octane.ImpinjReader
  Removes the diagnostic report listener.
removeDirectionReportListener() - Method in class com.impinj.octane.ImpinjReader
  Removes the direction report listener.
removeGpiChangeListener() - Method in class com.impinj.octane.ImpinjReader
  Removes the GPI change listener.
removeLocationReportListener() - Method in class com.impinj.octane.ImpinjReader
  Removes the location report listener.
removeResult(int) - Method in class com.impinj.octane.TagOpReport
removeSector(short) - Method in class com.impinj.octane.DirectionConfig
  Removes the specified sector from the list of sectors that should be monitored for tag entrances, exits, and updates.
removeTag(int) - Method in class com.impinj.octane.TagReport
removeTagOpCompleteListener() - Method in class com.impinj.octane.ImpinjReader
  Removes the tag operation listener.
removeTagReportListener() - Method in class com.impinj.octane.ImpinjReader
  Removes the tag report listener.
ReportConfig - Class in com.impinj.octane
  container class to specify the contents of tag Reports
ReportConfig() - Constructor for class com.impinj.octane.ReportConfig
ReportMode - Enum in com.impinj.octane
  The reader has several ways it can generate the tag reports that result from reader inventory operations.
resumeEventsAndReports() - Method in class com.impinj.octane.ImpinjReader
  This function tells the reader to resume sending reports and events.
RShellConnectionType - Enum in com.impinj.octane
  Enum used to specify the protocol over which the RShell connection will be made.
RshellEngine - Class in com.impinj.octane
  This class allows the application to generate rshell commands and process the rshell responses.
RshellEngine() - Constructor for class com.impinj.octane.RshellEngine
RshellReply - Class in com.impinj.octane
  This class helps the user parse and decode the tokens from a rshell reply.
RshellReply(String) - Constructor for class com.impinj.octane.RshellReply
  Contruct an Rshell Reply object from the response string from the rshell command
RShellSocket - Interface in com.impinj.octane
run() - Method in class com.impinj.octane.BackgroundWorker
run() - Method in class com.impinj.octane.ImpinjReader.MessageHandler
RxSensitivityTableEntry - Class in com.impinj.octane
  The reader can operate at different sensitivity levels to provide coarse control of the range of the device.
RxSensitivityTableEntry() - Constructor for class com.impinj.octane.RxSensitivityTableEntry

## S

save(String) - Method in class com.impinj.octane.FeatureSet
  writes the FeatureSet to a file
save(String) - Method in class com.impinj.octane.Settings
  Save the current settings object to a file in json
saveSettings() - Method in class com.impinj.octane.ImpinjReader
  Saves the settings object to a file in json format.
SearchMode - Enum in com.impinj.octane
  This enumeration describes the method the reader uses to search for tags.
SectorConfig - Class in com.impinj.octane
  Contains sector configuration for xArray.
SectorConfig() - Constructor for class com.impinj.octane.SectorConfig
send(String) - Method in class com.impinj.octane.RshellEngine
  Sends an rshell command to the reader
Send(String) - Method in interface com.impinj.octane.RShellSocket
Send(String) - Method in class com.impinj.octane.SshRShellSocket
Send(String) - Method in class com.impinj.octane.TelnetRShellSocket
SequenceState - Enum in com.impinj.octane
  Enumeration for defining the operation state for a sequence.
SequenceTriggerType - Enum in com.impinj.octane
  A tag operation sequence has a stop trigger that defines when the reader should stop executing the tag operation.
set(int, GpiConfig) - Method in class com.impinj.octane.GpiConfigGroup
set(int, GpoConfig) - Method in class com.impinj.octane.GpoConfigGroup
set_sectorId(short) - Method in class com.impinj.octane.SectorConfig
set_txFrequenciesInMhz(List<Double>) - Method in class com.impinj.octane.SectorConfig
  This is only applicable in regions that allow frequency control
setAccessPassword(TagData) - Method in class com.impinj.octane.TagBlockPermalockOp
setAccessPassword(TagData) - Method in class com.impinj.octane.TagLockOp
setAccessPassword(TagData) - Method in class com.impinj.octane.TagMarginReadOp
setAccessPassword(TagData) - Method in class com.impinj.octane.TagQtGetOp
setAccessPassword(TagData) - Method in class com.impinj.octane.TagQtSetOp
setAccessPassword(TagData) - Method in class com.impinj.octane.TagReadOp
setAccessPassword(TagData) - Method in class com.impinj.octane.TagWriteOp
setAccessPasswordLockType(TagLockState) - Method in class com.impinj.octane.TagLockOp
setAccessRange(QtAccessRange) - Method in class com.impinj.octane.TagQtGetOpResult
setAccessRange(QtAccessRange) - Method in class com.impinj.octane.TagQtSetOp
setAddress(String) - Method in class com.impinj.octane.ImpinjReader
  Sets the IP address or hostname of the reader.
setAntennaChangeListener(AntennaChangeListener) - Method in class com.impinj.octane.ImpinjReader
  The antenna change listener allows the application to receive antenna change reports from the reader
setAntennaConfigs(ArrayList<AntennaConfig>) - Method in class com.impinj.octane.AntennaConfigGroup
setAntennaCount(long) - Method in class com.impinj.octane.FeatureSet
setAntennaHubStatusGroup(AntennaHubStatusGroup) - Method in class com.impinj.octane.Status
setAntennaId(short) - Method in class com.impinj.octane.TagOpSequence
setAntennaPortNumber(short) - Method in class com.impinj.octane.Tag
setAntennaPortNumberPresent(boolean) - Method in class com.impinj.octane.Tag
setAntennas(AntennaConfigGroup) - Method in class com.impinj.octane.Settings
setAntennaStatusGroup(AntennaStatusGroup) - Method in class com.impinj.octane.Status
setAutoStart(AutoStartConfig) - Method in class com.impinj.octane.Settings
setAutoStop(AutoStopConfig) - Method in class com.impinj.octane.Settings
setBitCount(long) - Method in class com.impinj.octane.TagFilter
setBitCount(long) - Method in class com.impinj.octane.TagSelectFilter
setBitLength(int) - Method in class com.impinj.octane.MarginReadMask
  Set the bit length of the margin mask
setBitPointer(int) - Method in class com.impinj.octane.TagFilter
setBitPointer(int) - Method in class com.impinj.octane.TagMarginReadOp
setBitPointer(int) - Method in class com.impinj.octane.TagSelectFilter
setBitPointer(short) - Method in class com.impinj.octane.TargetTag
setBitPointer(short) - Method in class com.impinj.octane.TruncatedReplySettings
setBlockMask(BlockPermalockMask) - Method in class com.impinj.octane.TagBlockPermalockOp
  sets the mask of blocks to permanently lock
setBlockWrite(boolean) - Method in class com.impinj.octane.TagWriteOpResult
setBlockWriteEnabled(boolean) - Method in class com.impinj.octane.TagOpSequence
setBlockWriteRetryCount(short) - Method in class com.impinj.octane.TagOpSequence
setBlockWriteWordCount(short) - Method in class com.impinj.octane.TagOpSequence
setBufferOverflowListener(BufferOverflowListener) - Method in class com.impinj.octane.ImpinjReader
  The buffer overflow listener allows the application to receive a notification when the buffer in the reader has overflowed and tag reports and events may be getting lost
setBufferWarningListener(BufferWarningListener) - Method in class com.impinj.octane.ImpinjReader
  The buffer warning listener allows the application to receive a notification when the buffer has filled to TBD level.
setChannelInMhz(double) - Method in class com.impinj.octane.Tag
setChannelInMhzPresent(boolean) - Method in class com.impinj.octane.Tag
setComputeWindowSeconds(short) - Method in class com.impinj.octane.LocationConfig
  Compute Window the the smoothing window for averaging the location estimates.
setConfidenceFactors(LocationConfidenceFactors) - Method in class com.impinj.octane.LocationReport
setConnected(HubConnectedStatus) - Method in class com.impinj.octane.AntennaHubStatus
setConnected(boolean) - Method in class com.impinj.octane.AntennaStatus
setConnectionAttemptListener(ConnectionAttemptListener) - Method in class com.impinj.octane.ImpinjReader
  The connection attempt listener allows the application to receive a notification when other applications are trying to connect to the reader.
setConnectionCloseListener(ConnectionCloseListener) - Method in class com.impinj.octane.ImpinjReader
  The connection close listener allows the application to receive a notification when the reader has closed the connection to the SDK
setConnectionLostListener(ConnectionLostListener) - Method in class com.impinj.octane.ImpinjReader
  The connection list listener allows the application to receive a notification when the keepalives have stopped and the connection is presumed lost.
setConnectTimeout(int) - Method in class com.impinj.octane.ImpinjReader
  Set the connect timeout for all connection attempts with the reader.
setCrc(short) - Method in class com.impinj.octane.Tag
setCrcPresent(boolean) - Method in class com.impinj.octane.Tag
setData(List<Integer>) - Method in class com.impinj.octane.LocationConfidenceFactors
setData(TagData) - Method in class com.impinj.octane.TagReadOpResult
setData(TagData) - Method in class com.impinj.octane.TagWriteOp
setData(String) - Method in class com.impinj.octane.TargetTag
setDataProfile(QtDataProfile) - Method in class com.impinj.octane.TagQtGetOpResult
setDataProfile(QtDataProfile) - Method in class com.impinj.octane.TagQtSetOp
setDebounceInMs(long) - Method in class com.impinj.octane.GpiConfig
setDiagnosticReportEnabled(boolean) - Method in class com.impinj.octane.DirectionConfig
  When enabled, diagnostic reports are generated at each update interval and sent to the application
setDiagnosticReportEnabled(boolean) - Method in class com.impinj.octane.LocationConfig
  When enabled, diagnostic reports are generated at each update interval and sent to the application
setDiagnosticsReportListener(DiagnosticsReportListener) - Method in class com.impinj.octane.ImpinjReader
  Sets the diagnostic report listener.
setDirection(DirectionConfig) - Method in class com.impinj.octane.SpatialConfig
  Sets the reader's direction configuration.
setDirection(DirectionConfig) - Method in class com.impinj.octane.XArrayConfig
  Deprecated.
setDirectionReportListener(DirectionReportListener) - Method in class com.impinj.octane.ImpinjReader
  Set the direction report listener.
setDisabledAntennaList(List<Short>) - Method in class com.impinj.octane.LocationConfig
  Antennas can be disabled when configuring location.
setDisabledAntennaList(short[]) - Method in class com.impinj.octane.LocationConfig
  Antennas can be disabled when configuring location.
setDurationInMs(long) - Method in class com.impinj.octane.AutoStopConfig
setEmptyFieldTimeoutInMs(int) - Method in class com.impinj.octane.LowDutyCycleSettings
  When the reader detects and empty field (no tags) for this time, on a given antenna, it will enter low duty cycle mode and check this antenna for tags only periodically.
setEnabled(boolean) - Method in class com.impinj.octane.AntennaConfig
  An antenna can be enabled or disabled.
setEnabled(Boolean) - Method in class com.impinj.octane.KeepaliveConfig
setEnableLinkMonitorMode(Boolean) - Method in class com.impinj.octane.KeepaliveConfig
  In Link monitor mode, the reader will monitor keep alive responses from the SDk and close the connection if they are missed.
setEntryReportEnabled(boolean) - Method in class com.impinj.octane.DirectionConfig
  When enabled, an entry report is sent immediately upon the tag entering the field of view of the reader.
setEntryReportEnabled(boolean) - Method in class com.impinj.octane.LocationConfig
  When enabled, an entry report is sent immediately upon the tag entering the field of view of the reader.
setEpc(TagData) - Method in class com.impinj.octane.LocationReport
setEpc(TagData) - Method in class com.impinj.octane.Tag
setEpcLengthInWords(byte) - Method in class com.impinj.octane.TruncatedReplySettings
setEpcLockType(TagLockState) - Method in class com.impinj.octane.TagLockOp
setExecutionCount(short) - Method in class com.impinj.octane.TagOpSequence
setExitReportEnabled(boolean) - Method in class com.impinj.octane.DirectionConfig
  When enabled, an exit report is generated when the tag has not been seen by the reader in the tag age Interval.
setExitReportEnabled(boolean) - Method in class com.impinj.octane.LocationConfig
  When enabled, an exit report is generated when the tag has not been seen by the reader in the tag age Interval.
setFacilityXLocationCm(int) - Method in class com.impinj.octane.PlacementConfig
  When operating multiple xArrays in a single facility, a common coordinate system is desirable across all xArrays so that location data can be interpreted store-wide.
setFacilityYLocationCm(int) - Method in class com.impinj.octane.PlacementConfig
  When operating multiple xArrays in a single facility, a common coordinate system is desirable across all xArrays so that location data can be interpreted store-wide.
setFastIdAvailable(boolean) - Method in class com.impinj.octane.FeatureSet
setFastIdPresent(boolean) - Method in class com.impinj.octane.Tag
setFault(HubFaultStatus) - Method in class com.impinj.octane.AntennaHubStatus
setFieldOfView(DirectionFieldOfView) - Method in class com.impinj.octane.DirectionConfig
  Sets the field of view for tag direction tracking.
setFieldPingIntervalInMs(int) - Method in class com.impinj.octane.LowDutyCycleSettings
  When in low duty cycle mode, the reader will check the field for tags on each antenna at least once every Ping Interval.
setFilteringAvailable(boolean) - Method in class com.impinj.octane.FeatureSet
setFilterOp(TagFilterOp) - Method in class com.impinj.octane.TagFilter
setFilters(FilterSettings) - Method in class com.impinj.octane.Settings
setFirmwareVersion(String) - Method in class com.impinj.octane.FeatureSet
setFirstDelayInMs(long) - Method in class com.impinj.octane.AutoStartConfig
setFirstSeenTime(ImpinjTimestamp) - Method in class com.impinj.octane.Tag
setFirstSeenTimePresent(boolean) - Method in class com.impinj.octane.Tag
setGen2v2TagsOnly(boolean) - Method in class com.impinj.octane.TruncatedReplySettings
setGpiChangeListener(GpiChangeListener) - Method in class com.impinj.octane.ImpinjReader
  The GPI change listener allows the application to receive GPI change reports from the reader
setGpiCount(int) - Method in class com.impinj.octane.FeatureSet
setGpiDebounceAvailable(boolean) - Method in class com.impinj.octane.FeatureSet
setGpiLevel(Boolean) - Method in class com.impinj.octane.AutoStartConfig
setGpiLevel(Boolean) - Method in class com.impinj.octane.AutoStopConfig
setGpiPortNumber(int) - Method in class com.impinj.octane.AutoStartConfig
setGpiPortNumber(int) - Method in class com.impinj.octane.AutoStopConfig
setGpis(GpiConfigGroup) - Method in class com.impinj.octane.Settings
setGpiStatusGroup(GpiStatusGroup) - Method in class com.impinj.octane.Status
setGpo(int, boolean) - Method in class com.impinj.octane.ImpinjReader
  sets a GPO to specified state
setGpoCount(int) - Method in class com.impinj.octane.FeatureSet
setGpoPulseDurationMsec(long) - Method in class com.impinj.octane.GpoConfig
setGpos(GpoConfigGroup) - Method in class com.impinj.octane.Settings
setGpsCoodinates(GpsCoordinates) - Method in class com.impinj.octane.Tag
setGpsCoordinatesPresent(boolean) - Method in class com.impinj.octane.Tag
setHeightCm(short) - Method in class com.impinj.octane.PlacementConfig
  The xArray needs to know its height above ground level to perform location calculations.
setHoldReportsOnDisconnect(Boolean) - Method in class com.impinj.octane.Settings
  When the reader is running an inventory it may be collecting tag reports.
setHoppingRegion(boolean) - Method in class com.impinj.octane.FeatureSet
setHubId(short) - Method in class com.impinj.octane.AntennaHubStatus
setId(int) - Method in class com.impinj.octane.TagOpSequence
setImpinjRssiReportingAvailable(boolean) - Method in class com.impinj.octane.FeatureSet
setIncludeAntennaPortNumber(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludeChannel(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludeCrc(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludeDopplerFrequency(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludeFastId(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludeFirstSeenTime(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludeGpsCoordinates(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludeLastSeenTime(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludePcBits(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludePeakRssi(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludePhaseAngle(Boolean) - Method in class com.impinj.octane.ReportConfig
setIncludeSeenCount(Boolean) - Method in class com.impinj.octane.ReportConfig
setInterval(long) - Method in class com.impinj.octane.KeepaliveTimer
setIsConnected(boolean) - Method in class com.impinj.octane.Status
setIsEnabled(Boolean) - Method in class com.impinj.octane.GpiConfig
setIsEnabled(Boolean) - Method in class com.impinj.octane.LowDutyCycleSettings
setIsEnabled(boolean) - Method in class com.impinj.octane.TruncatedReplySettings
setIsMaxRxSensitivity(Boolean) - Method in class com.impinj.octane.AntennaConfig
  Typically an antenna is set to maximum sensitivity.
setIsMaxRxSensitivity(Boolean) - Method in class com.impinj.octane.AntennaConfigGroup
setIsMaxTxPower(Boolean) - Method in class com.impinj.octane.AntennaConfig
  Typically an antenna is set to maximum transmit power.
setIsMaxTxPower(Boolean) - Method in class com.impinj.octane.AntennaConfigGroup
setIsMaxTxPower(boolean) - Method in class com.impinj.octane.DirectionConfig
setIsMaxTxPower(Boolean) - Method in class com.impinj.octane.LocationConfig
  Typically an antenna is set to maximum transmit power.
setIsSingulating(boolean) - Method in class com.impinj.octane.Status
setKeepaliveListener(KeepaliveListener) - Method in class com.impinj.octane.ImpinjReader
  The keepalive listener allows the application to receive keepalive reports from the reader.
setKeepalives(KeepaliveConfig) - Method in class com.impinj.octane.Settings
setKeepaliveTimeoutListener(KeepaliveTimeoutListener) - Method in class com.impinj.octane.KeepaliveTimer
setKillPassword(TagData) - Method in class com.impinj.octane.TagKillOp
setKillPasswordLockType(TagLockState) - Method in class com.impinj.octane.TagLockOp
setLastSeenTime(ImpinjTimestamp) - Method in class com.impinj.octane.Tag
setLastSeenTimePresent(boolean) - Method in class com.impinj.octane.Tag
setLatitude(double) - Method in class com.impinj.octane.GpsCoordinates
setLinkDownThreshold(int) - Method in class com.impinj.octane.KeepaliveConfig
  In Link monitoring mode, this setting determines how many keep alives can be missed before the connection closes.
setLinkMonitorAvailable(boolean) - Method in class com.impinj.octane.FeatureSet
setLocation(LocationConfig) - Method in class com.impinj.octane.SpatialConfig
  Sets the reader's location configuration.
setLocation(LocationConfig) - Method in class com.impinj.octane.XArrayConfig
  Deprecated.
setLocationAlgorithmControlList(List<Integer>) - Method in class com.impinj.octane.LocationConfig
  Custom location algorithm control parameters can be set when configuring location.
setLocationAlgorithmControlList(int[]) - Method in class com.impinj.octane.LocationConfig
  Custom location algorithm control parameters can be set when configuring location.
setLocationReportListener(LocationReportListener) - Method in class com.impinj.octane.ImpinjReader
  Set the location report listener.
setLocationXCm(int) - Method in class com.impinj.octane.LocationReport
setLocationYCm(int) - Method in class com.impinj.octane.LocationReport
setLockResult(TagLockOpResult) - Method in class com.impinj.octane.LockTagResult
setLongitude(double) - Method in class com.impinj.octane.GpsCoordinates
setLowDutyCycle(LowDutyCycleSettings) - Method in class com.impinj.octane.Settings
setMarginMask(MarginReadMask) - Method in class com.impinj.octane.TagMarginReadOp
  sets the margin mask to compare the tag memory value against
setMask(String) - Method in class com.impinj.octane.TargetTag
setMaskFromBitString(String) - Method in class com.impinj.octane.MarginReadMask
  Sets the margin read mask from the specified bit string.
setMaskFromHexString(String) - Method in class com.impinj.octane.MarginReadMask
  Sets the margin read mask from the specified hex string.
setMatchingAction(TagFilterStateUnawareAction) - Method in class com.impinj.octane.TagSelectFilter
setMaxNumSelectFiltersPerQuery(int) - Method in class com.impinj.octane.FeatureSet
setMaxOperationSequences(int) - Method in class com.impinj.octane.FeatureSet
setMaxOperationsPerSequence(int) - Method in class com.impinj.octane.FeatureSet
setMaxRxSensitivity(boolean) - Method in class com.impinj.octane.SectorConfig
  Specifies that the maximum antenna receive sensitivity setting should be used.
setMaxTxPower(boolean) - Method in class com.impinj.octane.SectorConfig
  Specifies that the maximum antenna transmit power setting should be used.
setMemoryBank(MemoryBank) - Method in class com.impinj.octane.TagFilter
setMemoryBank(MemoryBank) - Method in class com.impinj.octane.TagMarginReadOp
setMemoryBank(MemoryBank) - Method in class com.impinj.octane.TagReadOp
setMemoryBank(MemoryBank) - Method in class com.impinj.octane.TagSelectFilter
setMemoryBank(MemoryBank) - Method in class com.impinj.octane.TagWriteOp
setMemoryBank(MemoryBank) - Method in class com.impinj.octane.TargetTag
setMessageTimeout(int) - Method in class com.impinj.octane.ImpinjReader
setMetrics(List<Integer>) - Method in class com.impinj.octane.DiagnosticReport
setMode(AutoStartMode) - Method in class com.impinj.octane.AutoStartConfig
setMode(AutoStopMode) - Method in class com.impinj.octane.AutoStopConfig
setMode(DirectionMode) - Method in class com.impinj.octane.DirectionConfig
setMode(TagFilterMode) - Method in class com.impinj.octane.FilterSettings
setMode(GpoMode) - Method in class com.impinj.octane.GpoConfig
setMode(ReportMode) - Method in class com.impinj.octane.ReportConfig
  The report Mode specifies when tag reports are generated
setMode(SpatialMode) - Method in class com.impinj.octane.SpatialConfig
  Sets the mode (Inventory, Location, or Direction) the reader with location or direction role capabilities is currently in.
setMode(XArrayMode) - Method in class com.impinj.octane.XArrayConfig
  Deprecated.
setModelDetails(TagModelDetails) - Method in class com.impinj.octane.Tag
setModelName(String) - Method in class com.impinj.octane.FeatureSet
setModelNumber(int) - Method in class com.impinj.octane.FeatureSet
setMultiwordBlockWriteAvailable(boolean) - Method in class com.impinj.octane.FeatureSet
setName(String) - Method in class com.impinj.octane.ImpinjReader
  Assigns a name to this reader.
setNonMatchingAction(TagFilterStateUnawareAction) - Method in class com.impinj.octane.TagSelectFilter
setNumWordsWritten(short) - Method in class com.impinj.octane.TagWriteOpResult
setOpId(short) - Method in class com.impinj.octane.TagOpResult
setOps(List<TagOp>) - Method in class com.impinj.octane.TagOpSequence
setOptimizedReadOps(ArrayList<TagReadOp>) - Method in class com.impinj.octane.ReportConfig
setOrientationDegrees(short) - Method in class com.impinj.octane.PlacementConfig
  When operating multiple xArrays in a single facility, a common coordinate system is desirable across all xArrays so that location data can be interpreted store-wide.
setPcBits(short) - Method in class com.impinj.octane.Tag
setPcBitsPresent(boolean) - Method in class com.impinj.octane.Tag
setPeakRssiInDbm(double) - Method in class com.impinj.octane.Tag
setPeakRssiInDbmPresent(boolean) - Method in class com.impinj.octane.Tag
setPercentFull(byte) - Method in class com.impinj.octane.BufferWarningEvent
setPeriodInMs(long) - Method in class com.impinj.octane.AutoStartConfig
  When using the periodic autostart trigger, the reader will initiate inventory periodically.
setPeriodInMs(long) - Method in class com.impinj.octane.KeepaliveConfig
setPersistence(QtPersistence) - Method in class com.impinj.octane.TagQtSetOp
setPhaseAngleInRadians(double) - Method in class com.impinj.octane.Tag
setPhaseAngleReportingAvailable(boolean) - Method in class com.impinj.octane.FeatureSet
setPlacement(PlacementConfig) - Method in class com.impinj.octane.SpatialConfig
  Sets the reader's placement configuration.
setPlacement(PlacementConfig) - Method in class com.impinj.octane.XArrayConfig
  Deprecated.
setPortName(String) - Method in class com.impinj.octane.AntennaConfig
  For convenience the antenna configuration hold a user defined port name.
setPortNumber(short) - Method in class com.impinj.octane.AntennaConfig
  Each antenna is identified by the port number to which this antenna configuration applies.
setPortNumber(short) - Method in class com.impinj.octane.AntennaEvent
setPortNumber(short) - Method in class com.impinj.octane.AntennaStatus
setPortNumber(int) - Method in class com.impinj.octane.GpiConfig
setPortNumber(short) - Method in class com.impinj.octane.GpiEvent
setPortNumber(short) - Method in class com.impinj.octane.GpiStatus
setPortNumber(int) - Method in class com.impinj.octane.GpoConfig
setReadCount(short) - Method in class com.impinj.octane.LocationConfidenceFactors
setReaderMode(ReaderMode) - Method in class com.impinj.octane.Settings
  Deprecated.
  The `ReaderMode` enum is no longer supported.

  Use `Settings.setRfMode(Integer)` instead. ReaderMode is the preselected set of gen2 physical layer settings to optimize tag communications for a certain scenario and environment

setReaderModel(ReaderModel) - Method in class com.impinj.octane.FeatureSet
setReaderModes(List<ReaderMode>) - Method in class com.impinj.octane.FeatureSet
  Deprecated.
  The `ReaderMode` enum is no longer supported.
setReaderStartListener(ReaderStartListener) - Method in class com.impinj.octane.ImpinjReader
  The reader start listener allows the application to receive a notification when the reader starts inventory
setReaderStopListener(ReaderStopListener) - Method in class com.impinj.octane.ImpinjReader
  The reader stop listener allows the application to receive a notification when the reader stops inventory
setReadOperationResults(List<TagReadOpResult>) - Method in class com.impinj.octane.Tag
setReducedPowerFrequenciesInMhz(ArrayList<Double>) - Method in class com.impinj.octane.Settings
setReport(ReportConfig) - Method in class com.impinj.octane.Settings
  Contains the configuration for Tag Reports
setReportType(LocationReportType) - Method in class com.impinj.octane.LocationReport
setResult(BlockPermalockResult) - Method in class com.impinj.octane.TagBlockPermalockOpResult
setResult(KillResultStatus) - Method in class com.impinj.octane.TagKillOpResult
setResult(LockResultStatus) - Method in class com.impinj.octane.TagLockOpResult
setResult(MarginReadResult) - Method in class com.impinj.octane.TagMarginReadOpResult
  Set the results of the margin read operation.
setResult(QtGetConfigResultStatus) - Method in class com.impinj.octane.TagQtGetOpResult
setResult(QtSetConfigResultStatus) - Method in class com.impinj.octane.TagQtSetOpResult
setResult(ReadResultStatus) - Method in class com.impinj.octane.TagReadOpResult
setResult(WriteResultStatus) - Method in class com.impinj.octane.TagWriteOpResult
setResults(List<TagOpResult>) - Method in class com.impinj.octane.TagOpReport
setRfDopplerFrequency(double) - Method in class com.impinj.octane.Tag
setRfDopplerFrequencyPresent(boolean) - Method in class com.impinj.octane.Tag
setRfMode(Integer) - Method in class com.impinj.octane.Settings
  RfMode is the preselected set of gen2 physical layer settings to optimize tag communications for a certain scenario and environment
setRfModes(List<Integer>) - Method in class com.impinj.octane.FeatureSet
setRfPhaseAnglePresent(boolean) - Method in class com.impinj.octane.Tag
setRxSensitivities(List<RxSensitivityTableEntry>) - Method in class com.impinj.octane.FeatureSet
setRxSensitivityinDbm(double) - Method in class com.impinj.octane.AntennaConfig
  Receive Sensitivity can be adjusted on the antenna to prevent the reader from receiving weak responses from tags.
setRxSensitivityinDbm(double) - Method in class com.impinj.octane.AntennaConfigGroup
setRxSensitivityInDbm(double) - Method in class com.impinj.octane.SectorConfig
  Defines the receive sensitivity in dBm (e.g.
setSearchMode(SearchMode) - Method in class com.impinj.octane.Settings
  Gen2 provides rudimentary building blocks to inventory populations of tags The Impinj reader creates high level inventory search modes from these gen2 operations.
setSeenCountPresent(boolean) - Method in class com.impinj.octane.Tag
setSequenceId(int) - Method in class com.impinj.octane.TagOpResult
setSequenceStopTrigger(SequenceTriggerType) - Method in class com.impinj.octane.TagOpSequence
setSerialNumber(String) - Method in class com.impinj.octane.FeatureSet
setSession(int) - Method in class com.impinj.octane.Settings
  Sets the gen2 session for the reader.
setSpatialConfig(SpatialConfig) - Method in class com.impinj.octane.Settings
  Sets the reader's settings object to be used to house configurations for readers with direction or location role capabilities.
setState(AntennaEventType) - Method in class com.impinj.octane.AntennaEvent
setState(boolean) - Method in class com.impinj.octane.GpiEvent
setState(boolean) - Method in class com.impinj.octane.GpiStatus
setState(SequenceState) - Method in class com.impinj.octane.TagOpSequence
setTag(Tag) - Method in class com.impinj.octane.TagOpResult
setTagAccessAvailable(boolean) - Method in class com.impinj.octane.FeatureSet
setTagAgeIntervalSeconds(short) - Method in class com.impinj.octane.DirectionConfig
  The "age interval" specifies how long a tag needs to go unseen before it's removed from the population of tags tracked for direction and an exit report is sent.
setTagAgeIntervalSeconds(short) - Method in class com.impinj.octane.LocationConfig
  The Age Interval specifies how long a tag needs to go unseen before its removed from the location tracking.
setTagFilter1(TagFilter) - Method in class com.impinj.octane.FilterSettings
setTagFilter2(TagFilter) - Method in class com.impinj.octane.FilterSettings
setTagMask(String) - Method in class com.impinj.octane.TagFilter
setTagMask(String) - Method in class com.impinj.octane.TagSelectFilter
setTagMask(String) - Method in class com.impinj.octane.TruncatedReplySettings
setTagOpCompleteListener(TagOpCompleteListener) - Method in class com.impinj.octane.ImpinjReader
  Sets the tag operation listener for the reader.
setTagPopulationEstimate(int) - Method in class com.impinj.octane.Settings
  When performing inventory operations, the Impinj reader uses the gen2 protocol's random access method to arbitrate between populations of tags.
setTagReportListener(TagReportListener) - Method in class com.impinj.octane.ImpinjReader
  Sets the tag report listener.
setTags(List<Tag>) - Method in class com.impinj.octane.TagReport
setTagSeenCount(short) - Method in class com.impinj.octane.Tag
setTagSelectFilterList(List<TagSelectFilter>) - Method in class com.impinj.octane.FilterSettings
  Set the tag select filter list.
setTargetTag(TargetTag) - Method in class com.impinj.octane.TagOpSequence
setTemperatureCelsius(short) - Method in class com.impinj.octane.Status
setTid(TagData) - Method in class com.impinj.octane.Tag
setTidLockType(TagLockState) - Method in class com.impinj.octane.TagLockOp
setTiltSensorValue(TiltSensorValue) - Method in class com.impinj.octane.Status
setTimeout(long) - Method in class com.impinj.octane.AutoStopConfig
setTimestamp(ImpinjTimestamp) - Method in class com.impinj.octane.LocationReport
Settings - Class in com.impinj.octane
  This is a container class for all of the knobs that control reader behavior.
setTruncatedReply(TruncatedReplySettings) - Method in class com.impinj.octane.Settings
setTxFrequencies(List<Double>) - Method in class com.impinj.octane.FeatureSet
setTxFrequenciesInMhz(ArrayList<Double>) - Method in class com.impinj.octane.Settings
setTxPowerinDbm(double) - Method in class com.impinj.octane.AntennaConfig
  Transmit power can be adjusted on the antenna to reduce the read range of the antenna.
setTxPowerinDbm(double) - Method in class com.impinj.octane.AntennaConfigGroup
setTxPowerinDbm(double) - Method in class com.impinj.octane.DirectionConfig
setTxPowerinDbm(double) - Method in class com.impinj.octane.LocationConfig
  Transmit power can be adjusted on antennas to reduce the read range of the antenna.
setTxPowerInDbm(double) - Method in class com.impinj.octane.SectorConfig
  Defines the antenna transmit power in dBm (e.g.
setTxPowers(List<TxPowerTableEntry>) - Method in class com.impinj.octane.FeatureSet
setUpdateIntervalSeconds(short) - Method in class com.impinj.octane.DirectionConfig
  Specifies how often update reports are sent when updates are enabled.
setUpdateIntervalSeconds(short) - Method in class com.impinj.octane.LocationConfig
  The ReportInterval specifies how often tag reports are generated when tag report updates are enabled
setUpdateReportEnabled(boolean) - Method in class com.impinj.octane.DirectionConfig
setUpdateReportEnabled(boolean) - Method in class com.impinj.octane.LocationConfig
setUserLockType(TagLockState) - Method in class com.impinj.octane.TagLockOp
setUserTagPopulationLimit(short) - Method in class com.impinj.octane.DirectionConfig
setUtcTimestamp(long) - Method in class com.impinj.octane.AutoStartConfig
  TODO
setWordCount(short) - Method in class com.impinj.octane.TagReadOp
setWordPointer(short) - Method in class com.impinj.octane.TagReadOp
setWordPointer(short) - Method in class com.impinj.octane.TagWriteOp
setXArray(XArrayConfig) - Method in class com.impinj.octane.Settings
  Deprecated.
setxAxis(int) - Method in class com.impinj.octane.TiltSensorValue
setyAxis(int) - Method in class com.impinj.octane.TiltSensorValue
SpatialConfig - Class in com.impinj.octane
  Class used to define the configuration for a reader with location or direction role capabilities.
SpatialMode - Enum in com.impinj.octane
  An enumeration to describe a reader with direction or location role capabilities' operational mode.
SshRShellSocket - Class in com.impinj.octane
SshRShellSocket(String, String, String, int) - Constructor for class com.impinj.octane.SshRShellSocket
start() - Method in class com.impinj.octane.ImpinjReader
  Starts the reader.
start() - Method in class com.impinj.octane.KeepaliveTimer
  starts the keep alive timer
Status - Class in com.impinj.octane
  The status class holds information on the current status of reader functions.
Status() - Constructor for class com.impinj.octane.Status
stop() - Method in class com.impinj.octane.ImpinjReader
  Stops the reader from its inventory.
stop() - Method in class com.impinj.octane.KeepaliveTimer
  stops the keep alive timer

## T

Tag - Class in com.impinj.octane
  A container class to hold information about a tag.
Tag() - Constructor for class com.impinj.octane.Tag
  construct a new tag object
TagBlockPermalockOp - Class in com.impinj.octane
  Used to perform a block permalock operation on a tag
TagBlockPermalockOp() - Constructor for class com.impinj.octane.TagBlockPermalockOp
TagBlockPermalockOpResult - Class in com.impinj.octane
  Used to report the status of a block permalock operations
TagBlockPermalockOpResult() - Constructor for class com.impinj.octane.TagBlockPermalockOpResult
TagData - Class in com.impinj.octane
  A class to hold tag data including EPCs, user memory data, TID memory etc.
TagData() - Constructor for class com.impinj.octane.TagData
TagFilter - Class in com.impinj.octane
  A class to hold the configuration of a tag inventory filter.
TagFilter() - Constructor for class com.impinj.octane.TagFilter
TagFilterMode - Enum in com.impinj.octane
  enumerates the different ways the two tag filters can be combined during the inventory operation
TagFilterOp - Enum in com.impinj.octane
  What to do when comparing tag filters against the data patterns
TagFilterStateUnawareAction - Enum in com.impinj.octane
  The action to perform when tag filter matches or doesn't match
TagKillOp - Class in com.impinj.octane
  Class used to specify a tag kill operation.
TagKillOp() - Constructor for class com.impinj.octane.TagKillOp
TagKillOpResult - Class in com.impinj.octane
  Class to contain the results of a tag Kill operation
TagKillOpResult() - Constructor for class com.impinj.octane.TagKillOpResult
TagLockOp - Class in com.impinj.octane
  Class to contain the information to perform a tag Lock operation.
TagLockOp() - Constructor for class com.impinj.octane.TagLockOp
TagLockOpResult - Class in com.impinj.octane
  Class to contain the results of a tag lock operation
TagLockOpResult() - Constructor for class com.impinj.octane.TagLockOpResult
TagLockState - Enum in com.impinj.octane
  An enumeration for determining which lock operation to perform on the tag memory bank; this determines what state to leave the tag memory bank in.
TagMarginReadOp - Class in com.impinj.octane
  Used to perform a margin read operation on a tag
TagMarginReadOp() - Constructor for class com.impinj.octane.TagMarginReadOp
TagMarginReadOpResult - Class in com.impinj.octane
  Used to report the status of margin read operations
TagMarginReadOpResult() - Constructor for class com.impinj.octane.TagMarginReadOpResult
TagModelDetails - Class in com.impinj.octane
  A class that decodes the tag model details from the TID memory read
TagModelDetails() - Constructor for class com.impinj.octane.TagModelDetails
TagModelDetails(String) - Constructor for class com.impinj.octane.TagModelDetails
TagModelName - Enum in com.impinj.octane
  an enumeration to contain the tag model names.
TagOp - Class in com.impinj.octane
  A base class to hold information to perform a tag operation like read, write, lock, and kill.
TagOp() - Constructor for class com.impinj.octane.TagOp
TagOpCompleteListener - Interface in com.impinj.octane
  Your application can implement this interface to receive tag operation events.
TagOpReport - Class in com.impinj.octane
  Container class used to encapsulate all tag operation results.
TagOpReport() - Constructor for class com.impinj.octane.TagOpReport
TagOpResult - Class in com.impinj.octane
  Parent class that contains the results of an individual tag operation
TagOpResult() - Constructor for class com.impinj.octane.TagOpResult
TagOpSequence - Class in com.impinj.octane
  Class for containing and configuring a sequence of tag operations that are submitted to the reader
TagOpSequence() - Constructor for class com.impinj.octane.TagOpSequence
TagQtGetOp - Class in com.impinj.octane
  A class to contain the QT get operation
TagQtGetOp() - Constructor for class com.impinj.octane.TagQtGetOp
TagQtGetOpResult - Class in com.impinj.octane
  A class to contain the QtGetOp result
TagQtGetOpResult() - Constructor for class com.impinj.octane.TagQtGetOpResult
TagQtSetOp - Class in com.impinj.octane
  A class to contain the QTSet operation data
TagQtSetOp() - Constructor for class com.impinj.octane.TagQtSetOp
TagQtSetOpResult - Class in com.impinj.octane
  a class to contain the results of a qt set operation
TagQtSetOpResult() - Constructor for class com.impinj.octane.TagQtSetOpResult
TagReadOp - Class in com.impinj.octane
  A class to contain the data for a tag read operation
TagReadOp() - Constructor for class com.impinj.octane.TagReadOp
TagReadOpResult - Class in com.impinj.octane
  a class to contain the read operation results
TagReadOpResult() - Constructor for class com.impinj.octane.TagReadOpResult
TagReport - Class in com.impinj.octane
  a container class to carry a tag report
TagReport() - Constructor for class com.impinj.octane.TagReport
TagReportListener - Interface in com.impinj.octane
  Your application can implement this interface to receive tag report events.
TagSelectFilter - Class in com.impinj.octane
  A class to hold the configuration of an inventory select command.
TagSelectFilter() - Constructor for class com.impinj.octane.TagSelectFilter
TagWriteOp - Class in com.impinj.octane
  A class to contain the data for a tag write operation
TagWriteOp() - Constructor for class com.impinj.octane.TagWriteOp
TagWriteOpResult - Class in com.impinj.octane
  A class to contain the results of a tag write operation
TagWriteOpResult() - Constructor for class com.impinj.octane.TagWriteOpResult
TargetTag - Class in com.impinj.octane
  Helper class used to identify a specific tag or set of tags on which to perform a tag operation operation.
TargetTag() - Constructor for class com.impinj.octane.TargetTag
TelnetRShellSocket - Class in com.impinj.octane
TelnetRShellSocket(String, String, String, int) - Constructor for class com.impinj.octane.TelnetRShellSocket
TiltSensorValue - Class in com.impinj.octane
  Holds the X, Y, and Z values returned by the tilt sensor.
TiltSensorValue() - Constructor for class com.impinj.octane.TiltSensorValue
toDoubleWord() - Method in class com.impinj.octane.TagData
  Returns the value of a TagData object as a long integer
toHexString() - Method in class com.impinj.octane.MarginReadMask
  Converts the margin read mask into a hexadecimal string.
toHexString(short) - Static method in class com.impinj.octane.PcBits
  formats the EPC bits as a hex string.
toHexString() - Method in class com.impinj.octane.TagData
  Returns the value of a TagData object as a hexadecimal string
toHexWordString() - Method in class com.impinj.octane.BlockPermalockMask
  Converts the block permalock mask into a hexadecimal string.
toHexWordString() - Method in class com.impinj.octane.MarginReadMask
  Converts the margin read mask into a hexadecimal string with spaces between words.
toHexWordString() - Method in class com.impinj.octane.TagData
  Returns the value of a TagData object as a hexadecimal string with each 16-bit word separated by a space
toImpinjDirectionReportType() - Method in enum com.impinj.octane.DirectionReportType
toString() - Method in class com.impinj.octane.DirectionReport
toString() - Method in enum com.impinj.octane.DirectionReportType
ToString() - Method in class com.impinj.octane.GpsCoordinates
  Override of the ToString operator that concatenates the Latitude and Longitude parameters into a single string.
toString() - Method in class com.impinj.octane.ImpinjReader
ToString() - Method in class com.impinj.octane.ImpinjTimestamp
  Conversion utility that outputs the ImpinjTimestamp data as a string.
toString() - Method in class com.impinj.octane.TagData
  Returns the value of a TagData object as a hexadecimal string
toWordList() - Method in class com.impinj.octane.TagData
  Returns the value of a TagData object as a List of Integers
TruncatedReplySettings - Class in com.impinj.octane
  Class containing the settings for using Truncated Reply during Inventory.
TruncatedReplySettings() - Constructor for class com.impinj.octane.TruncatedReplySettings
tryToStop() - Method in class com.impinj.octane.BackgroundWorker
turnBeaconOff() - Method in class com.impinj.octane.ImpinjReader
  Turns off the xArray beacon LED
turnBeaconOn(long) - Method in class com.impinj.octane.ImpinjReader
  Turns on the xArray Beacon LED.
txFrequencies - Variable in class com.impinj.octane.FeatureSet
TxPowerTableEntry - Class in com.impinj.octane
  a class to contain a list of available transmit power options
TxPowerTableEntry() - Constructor for class com.impinj.octane.TxPowerTableEntry

## V

valueOf(String) - Static method in enum com.impinj.octane.AntennaEventType
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.AntennaEventType
valueOf(String) - Static method in enum com.impinj.octane.AutoStartMode
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.AutoStartMode
valueOf(String) - Static method in enum com.impinj.octane.AutoStopMode
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.AutoStopMode
valueOf(String) - Static method in enum com.impinj.octane.BlockPermalockResult
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.BlockPermalockResult
valueOf(String) - Static method in enum com.impinj.octane.CommunicationsStandardType
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.impinj.octane.ConnectAsyncResult
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.impinj.octane.DirectionFieldOfView
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.impinj.octane.DirectionMode
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.impinj.octane.DirectionReportType
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.DirectionReportType
valueOf(String) - Static method in enum com.impinj.octane.DirectionTagPopulationStatus
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.DirectionTagPopulationStatus
valueOf(String) - Static method in enum com.impinj.octane.GpoMode
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.GpoMode
valueOf(String) - Static method in enum com.impinj.octane.HubConnectedStatus
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.HubConnectedStatus
valueOf(String) - Static method in enum com.impinj.octane.HubFaultStatus
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.HubFaultStatus
valueOf(String) - Static method in enum com.impinj.octane.KillResultStatus
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.KillResultStatus
  translates the interger value into an enumeration object
valueOf(String) - Static method in enum com.impinj.octane.LocationReportType
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.LocationReportType
valueOf(String) - Static method in enum com.impinj.octane.LockMemoryBank
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.LockMemoryBank
valueOf(String) - Static method in enum com.impinj.octane.LockResultStatus
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.LockResultStatus
valueOf(String) - Static method in enum com.impinj.octane.LockType
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.LockType
valueOf(String) - Static method in enum com.impinj.octane.MarginReadResult
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.MarginReadResult
valueOf(String) - Static method in enum com.impinj.octane.MemoryBank
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.MemoryBank
valueOf(String) - Static method in enum com.impinj.octane.QtAccessRange
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.QtAccessRange
valueOf(String) - Static method in enum com.impinj.octane.QtDataProfile
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.QtDataProfile
valueOf(String) - Static method in enum com.impinj.octane.QtGetConfigResultStatus
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.QtGetConfigResultStatus
  Return the qtGetConfiguResult for a given integer value
valueOf(String) - Static method in enum com.impinj.octane.QtPersistence
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.QtPersistence
valueOf(String) - Static method in enum com.impinj.octane.QtSetConfigResultStatus
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.QtSetConfigResultStatus
valueOf(String) - Static method in enum com.impinj.octane.ReaderMode
  Deprecated.
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.ReaderMode
  Deprecated.
valueOf(String) - Static method in enum com.impinj.octane.ReaderModel
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.ReaderModel
valueOf(String) - Static method in enum com.impinj.octane.ReadResultStatus
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.ReadResultStatus
valueOf(String) - Static method in enum com.impinj.octane.ReportMode
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.ReportMode
valueOf(String) - Static method in enum com.impinj.octane.RShellConnectionType
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.impinj.octane.SearchMode
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.SearchMode
valueOf(String) - Static method in enum com.impinj.octane.SequenceState
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.SequenceState
valueOf(String) - Static method in enum com.impinj.octane.SequenceTriggerType
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.SequenceTriggerType
valueOf(String) - Static method in enum com.impinj.octane.SpatialMode
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.impinj.octane.TagFilterMode
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.impinj.octane.TagFilterOp
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.impinj.octane.TagFilterStateUnawareAction
  Returns the enum constant of this type with the specified name.
valueOf(String) - Static method in enum com.impinj.octane.TagLockState
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.TagLockState
valueOf(String) - Static method in enum com.impinj.octane.TagModelName
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.TagModelName
  The TID is the second word of the 2-word TID read from user memory as an 16-bit integer.
valueOf(String) - Static method in enum com.impinj.octane.WriteResultStatus
  Returns the enum constant of this type with the specified name.
valueOf(int) - Static method in enum com.impinj.octane.WriteResultStatus
valueOf(String) - Static method in enum com.impinj.octane.XArrayMode
  Deprecated.
  Returns the enum constant of this type with the specified name.
values() - Static method in enum com.impinj.octane.AntennaEventType
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.AutoStartMode
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.AutoStopMode
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.BlockPermalockResult
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.CommunicationsStandardType
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.ConnectAsyncResult
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.DirectionFieldOfView
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.DirectionMode
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.DirectionReportType
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.DirectionTagPopulationStatus
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.GpoMode
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.HubConnectedStatus
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.HubFaultStatus
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.KillResultStatus
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.LocationReportType
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.LockMemoryBank
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.LockResultStatus
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.LockType
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.MarginReadResult
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.MemoryBank
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.QtAccessRange
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.QtDataProfile
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.QtGetConfigResultStatus
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.QtPersistence
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.QtSetConfigResultStatus
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.ReaderMode
  Deprecated.
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.ReaderModel
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.ReadResultStatus
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.ReportMode
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.RShellConnectionType
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.SearchMode
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.SequenceState
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.SequenceTriggerType
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.SpatialMode
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.TagFilterMode
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.TagFilterOp
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.TagFilterStateUnawareAction
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.TagLockState
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.TagModelName
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.WriteResultStatus
  Returns an array containing the constants of this enum type, in the order they are declared.
values() - Static method in enum com.impinj.octane.XArrayMode
  Deprecated.
  Returns an array containing the constants of this enum type, in the order they are declared.

## W

WordPointers - Class in com.impinj.octane
  Helper class used when defining tag memory accesses.that use word pointers
WordPointers() - Constructor for class com.impinj.octane.WordPointers
workOn(Method) - Method in class com.impinj.octane.BackgroundWorker
WriteResultStatus - Enum in com.impinj.octane
  a enumeration to report the results of a write operation

## X

XArrayConfig - Class in com.impinj.octane
  Deprecated.
XArrayConfig() - Constructor for class com.impinj.octane.XArrayConfig
  Deprecated.
XArrayMode - Enum in com.impinj.octane
  Deprecated.

A B C D E F G H I K L M O P Q R S T V W X